## Retrospect 5.11 for Windows

### HTML-format Read Me, updated March 14, 2000

This hypertext document contains important information about Retrospect version 5.11 for Windows. Please read this document carefully. The Retrospect family of backup software includes Retrospect Desktop Backup, Retrospect Workgroup Backup, and Retrospect Server Backup. Unless otherwise noted, all items in this document refer to all members of the Retrospect backup family.

The Dantz web site is constantly updated with the most recent support information for Retrospect and related products, including the following:

- latest read me file, which includes the latest list of supported devices
- technical support
- upgrades
- updates

This document is divided into the following sections:

1. Tips and Late-Breaking Information
2. Windows Client Conflicts and Workarounds
3. Macintosh Client Conflicts and Workarounds
4. Hardware Conflicts and Workarounds
5. Supported Devices

## Tips and Late-Breaking Information

License Codes: Retrospect requires a license code to function. The first time you start Retrospect, enter the license code.

If you purchased your Retrospect software for electronic download, your license code should be e-mailed to you by your vendor; if you did not receive the code, contact your vendor. Write down or print out your license code for future reference and keep the code in a safe place. Without this license code, you will not be able to use your Retrospect software.

Adding a Backup Device: When you install a new backup device on your computer, you may need to take some extra steps to satisfy Windows' Add New Hardware wizard. If you are installing a CD-R or CD-RW device or a new removable device such as a Zip, Jaz, DVD-RAM, or SuperDisk, follow the instructions included with it to install required device drivers. If you are installing a tape drive, follow the appropriate steps below, according to your operating system. No action is required for Windows NT 4.0.

- Windows 95
  After installing the tape drive, turn on the computer and the Add New Hardware wizard appears during startup. If it does not automatically find a driver for your new device, select "Do not install a driver (Windows will not prompt you again)" and click OK.
- Windows 98 and 2000
  After installing the tape drive, turn on the computer and the Add New Hardware wizard appears during startup. If it does not automatically find a driver for your new device, first select "Search for the best driver for your device (recommended)" and click OK. Then, in the Search selection dialog, select only the floppy disk drive as the search destination. When the wizard reports "Windows was unable to locate a driver for this device," click Next to continue. When the wizard reports "Windows has not installed a driver for this device," click Finish.

Windows 2000 Support: Retrospect 5.1 offers full support for Windows 2000 Professional and extensive support for Windows 2000 Server. Windows 2000 Server support includes backup and restore of Active Directory, COM+, and Certificate Server databases. Support for Windows 2000 is fully documented in the Retrospect 5.1 User's Guide Addendum.

## Windows Client Conflicts and Workarounds

Windows Socket 2 Update for Windows 95: Windows 95 clients require the Windows Socket 2 Update, available at no charge from Microsoft. Known as Winsock2, it is required only for Windows 95, and is available free from Microsoft's web site.

Microsoft Windows 95 TCP/IP Fix: A bug in Windows 95 networking software can cause Retrospect to report a networking error. Microsoft has resolved this problem and a free fix is available from Microsoft. Windows 98, Windows NT 4.0, and Windows 2000 do not require an update. We strongly urge you to update your Windows 95 systems.

The hot fix for Windows 95 is installed by the client software Setup program. After installation, choose Run from the Start menu, then type "C:\Program Files\Dantz\Client\VTCPUPD" (or your different installation path) and click OK. Follow the instructions in Microsoft's installer, then restart to complete the fix. Repeat for each Windows 95 computer to be used with Retrospect.

The problem can occur when Retrospect pauses then later resumes a TCP/IP network transfer. For example, it can happen when Retrospect requests media during the nightly backup and you insert a new tape the next morning. The bug can cause Retrospect to report error -519 (network communication failed) when it resumes a paused transfer.

Suspend: If you or a client user uses the "Suspend" function of Windows 95, which powers off a mobile computer without shutting it down, you must restart the client computer before Retrospect can access it. Microsoft has an update to address this problem, but Microsoft does not recommend updating unless you are severely impacted by it. For more information about this problem and the update, visit Microsoft's web page. This problem is resolved in Microsoft Windows 98.

## Macintosh Client Conflicts and Workarounds

AppleShare 4.2.1: When restoring or duplicating files to an AppleShare file server disk, some copied applications can be assigned incorrect type and creator codes, such as BINA and pdos. This is caused by a bug, which is fixed in AppleShare IP 5.0 and later.

First Class server: To avoid problems with a First Class server, close down the First Class server before backing it up. With a version earlier than 3.5, also run the utility to update the Post Office Map. This avoids errors with backups and ensures the server can be restored.

AccessPC: If you use AccessPC on a Macintosh which you plan to back up using Retrospect client software, rename the °Retrospect Client control panel file by replacing the "°" with a space. When the client Macintosh starts up, the renamed control panel loads before AccessPC, ensuring compatibility.

Apple Ethernet drivers on beige G3 Macs: Apple's beige G3 Ethernet drivers version 2.0, 2.0.1, 2.0.2, and 2.0.3 drivers have a problem that can cause network backup failures and loss of network services when using the built-in Ethernet interface of beige G3 desktop and mini-towers (but not PowerBook G3). Apple fixed the problem with version 2.0.4 of its built-in Ethernet software. If you experience network backup trouble on beige G3 computers you should update your driver. You can learn more about and download the latest driver from Apple.

At Ease for Workgroups: When backing up a server running At Ease for Workgroups, Retrospect may report error -54 (file busy/locked) when copying the following At Ease files: setups.data, setups.idx, Users.data, Users.idx.

AutoDoubler: For best compatibility, use version 2.0.6 or later, which is part of Norton DiskDoubler Pro 1.1.3. If you have questions about AutoDoubler, contact Symantec at 541.465.8440 or 800.441.7234. During the compare pass of a duplicate operation Retrospect reports a data offset error at byte 40 for a number of AutoDoubler-compressed files. This is caused by an AutoDoubler bug in which it does not set the BNDL bit of compressed applications. It is important to understand that the data is not corrupt and that the issue is only cosmetic. Use a program such as Norton Utilities to fix affected applications.

Energy Saver: Apple's Energy Saver control panel can put a non-PCI client Macintosh into "sleep" mode, which may produce error -530 with network backups. Avoid this problem by using the Retrospect Client control panel's "Wait at Shutdown" preference and shutting down the client to put it in the "waiting for backup" mode, or by setting the CPU sleep option to never sleep.

General Controls: Early versions of the General Controls control panel included with System 7.5 sometimes caused Retrospect to report error -15276 or error -15277. To avoid these errors, update your system software to version 7.5.3 or later.

Launcher: To avoid conflicts concerning the bullet character (Option-8) in folder names, client Macintosh computers using the Private Files/Folders/Volumes preference should use aliases in the Launcher Items folder. After a restore, you may need to manually rebuild the Launcher Items folder. Any time you use the Private Files/Folders/Volumes preference, you must ensure only files not desired for backup are restricted by the bullet character. This includes folders enclosing files.

Mac OS Extended Format (HFS+) Time Zone: When the local time zone is changed in the Date & Time control panel, the Mac OS shifts the local creation and modification times of files on HFS+ (extended format) volumes. This affects Retrospect's normal backups when it scans the volumes for files which need to be backed up. Because file date/time stamps are different, Retrospect marks every file for backup. Retrospect is simply performing an incremental backup as it usually would; the only abnormality is that every file appears to have been modified. For more information regarding HFS+ date/time stamps, refer to Dantz Technical Note 405, "Effects of HFS+ on Retrospect when Standard or Daylight Savings Time Changes."

Mac OS Extended Format (HFS+) Daylight Savings Time: Under Mac OS 8.1, changing the Daylight Savings time setting shifts the local dates and times of files on HFS+ volumes. This affects Retrospect as described in the previous topic. Mac OS 8.5 solves this problem because it does not alter file date/time stamps when you change Daylight Savings in the Date & Time control panel. For more information regarding HFS+ date/time stamps, refer to Dantz Technical Note 405.

Microsoft Mail: Microsoft Mail 3.0 and 3.1 data files on an MS Mail workstation often become corrupted. MS Mail 3.1a data files become corrupted when the workstation's mail application is open while Retrospect backs it up. Update to version 3.1a and implement a custom Selector with Retrospect that excludes busy MS Mail data files.

Microsoft Office Manager: A bug in the Microsoft Office Manager (MOM) extension causes the Finder to hang or prevents shutdown when Retrospect is scanning the volume. Update to version 4.2.1c, part of Microsoft's Office update for Power Macintosh.

Now QuickFiler (formerly Now Compress): For best compatibility, use version 5.0.2 or later and set it to compress individual volumes rather than all volumes. If you have questions about Now QuickFiler contact Power On Software.

RAM Doubler: You must use version 2.0.1 with System 7.5.5 or later.

Speed Doubler: You must use version 1.1 or later. Prior versions may result in hangs during restore operations with large volumes.

Some specialized accounting software: To ensure the integrity of backups for the MediMac®, DentalMac®, ChiroMac®, and Great Plains accounting systems, back up as described on page 159 of the Retrospect User's Guide, under "Programs Which Do Not Update File Dates." To restore your accounting data, always use the "Restore an entire disk" option to restore the Snapshot of the accounting Subvolume to a new, empty Subvolume.

Asante 10/100 Ethernet card: A bug in this network card causes the Macintosh to hang with TCP/IP. Asante's version 2.4 or later of the Mac 10/100 driver takes care of the problem with the card. The new driver disk image is posted on Asante's web site.

PowerBook 3400: A PowerBook 3400 TCP/IP Retrospect client may halt network communication during a backup. Retrospect reports an error -519 as the PowerBook's networking stops. (You will find both TCP/IP and AppleTalk networking non-functional until you restart the computer.) Apple has provided a software fix, which you can learn more about and download from Apple. Upgrading to Mac OS 8.1 also fixes the problem.

Mac OS clients don't renew DHCP leases while waiting for shutdown: When a Mac OS TCP/IP Retrospect client has a DHCP-supplied IP address and its lease expires while the client is waiting for shutdown, the Mac does not renew its IP lease and continues using its old IP address. This can lead to a conflict when the DHCP server, thinking the IP address is now available, leases the IP address to a different computer.

There are two possible workarounds: leave DHCP-served Mac OS computers idle in the Finder instead of in the Retrospect client "Wait at Shutdown" mode and uncheck "Load Only When Needed" in the TCP/IP control panel; or, lengthen your DHCP server's lease period. The likelihood of encountering this problem decreases as the length of DHCP leases increases.

## Hardware Conflicts and Workarounds

Windows NT 4.0 and ATAPI devices: Windows NT 4.0 Service Pack 3 and later greatly improve compatibility with ATAPI storage devices. If you are encountering problems with an ATAPI storage device, contact the computer vendor for a new IDE controller driver.

Removable Storage Management: Windows 2000's Removable Storage management console allows you to manage tape libraries and other storage devices in conjunction with the operating system's built-in backup utility. Because this interferes with Retrospect's access of those same devices, Retrospect automatically disables the Removable Storage service when it scans the SCSI bus for devices.With the service disabled, you cannot use the Removable Storage management console.

DVD-RAM Drives: Retrospect will not recognize a DVD-RAM drive if a DVD-RAM disk was not in the drive before Retrospect scanned for available backup devices. If the DVD-RAM drive is not visible in Retrospect's media request window, check whether Windows Explorer shows a drive letter for a removable disk in My Computer. If the DVD-RAM drive has a letter in Windows Explorer but it is not in the media request window, click Device Status to open the device status window, then click Refresh.

Write DVD! Driver: When this driver from Software Architects is in use, Retrospect cannot eject DVD-RAM disks because the driver intercepts eject requests. Use Windows Explorer to eject media.

DirectCD: Retrospect is not able to access a CD-R or CD-RW device if an Adaptec DirectCD-formatted disc is in the drive. Eject all DirectCD volumes from the CD-R or CD-RW drive before opening Retrospect.

Removable Disks: If you are using a removable disk drive under Windows NT, format your disks as NTFS, unless you need to keep them FAT to share data with others. Erasing FAT volumes for use with Retrospect takes longer than erasing NTFS volumes.

Imation LS-120 SuperDisk: Retrospect will not recognize a SuperDisk drive if a 1.4 M floppy disk was in the drive before Retrospect scanned for available backup devices. If the SuperDisk drive is not visible in Retrospect's media request window, check whether Windows Explorer shows a drive letter for a removable disk in My Computer. If the SuperDisk drive has a letter in Windows Explorer but it is not in the media request window, click Device Status to open the device status window, then click Refresh.

Auto-Ejecting Removable Disks: Windows 95 and 98 may give you a blue screen error message when Retrospect automatically ejects a removable disk. To prevent this, go to Special>Preferences>Media>Handling and turn on the Don't eject removable disks preference.

## Supported Devices

These notes provide information regarding Retrospect and specific storage devices. For details on communication buses and hardware, refer to the Retrospect User's Guide, Chapter 3 · Hardware.

Drives listed in these notes have been extensively tested and qualified for use with Retrospect by Dantz. If your drive's mechanism is not mentioned it may be supported by a new version of Retrospect or a driver update posted on the Dantz web site. If your drive is not supported and it is an old drive, it may not be qualified by Dantz. If you have questions about support for your drive contact Dantz Technical Support.

These notes on backup devices are divided into categories by the type of mechanism and media used by each drive. To find the name of your drive mechanism, click the Devices button on the Retrospect Directory's Configure tab. To get additional device identification information for any type of drive, click the Device Status button.

- Firmware
- Removable Drives
- CD-R and CD-RW Drives
- Tape Drives
- Libraries

### Firmware

Certain drives require specific versions of firmware, the drive's built-in controlling software. To determine your drive's firmware version, click Retrospect's Configure tab, click Devices, and click the Device Status button. If your firmware is an earlier version than is required, contact your drive vendor.

### Removable Drives

Retrospect supports all drives which are accessible from Windows Explorer. This includes removable cartridge drives from Iomega and SyQuest, Imation's SuperDisk, DVD-RAM drives from Hitachi, Panasonic, and Toshiba, and magneto-optical drives from Epson, Fujitsu, Mitsubishi Chemical, Olympus, Philips, Pinnacle, Ricoh, Sony, and others. Retrospect uses no more than 2 GB per side, even if there is more space available on the disk.

### CD-R and CD-RW Drives

Supported CD-R and CD-RW Mechanisms
Mechanism | Type | Capacity | Comments
--- | --- | --- | ---
Acer CRW620 | CD-RW | 610 MB | Requires firmware version 1.20.
Actima ARW4420S | CD-RW | 610 MB |
AOpen CRW9420S | CD-RW | 610 MB |
Artmedia RW6220B | CD-RW | 610 MB |
BTC RW6220BT | CD-RW | 610 MB |
Delta OIP-RW2004/B | CD-RW | 610 MB |
HP CD-Writer Plus 8100 series | CD-RW | 610 MB |
HP CD-Writer Plus 8200 series | CD-RW | 610 MB |
HP CD-Writer Plus M820e | CD-RW | 610 MB |
HP CD-Writer Plus 9100 Series | CD-RW | 610 MB |
HP CD-Writer Plus 9200 Series | CD-RW | 610 MB |
Imation IMR080020 CD SuperRecorder | CD-R | 610 MB |
Imation IMW080220 CD-RW SuperRecorder | CD-RW | 610 MB |
Iomega Zip CD | CD-RW | 610 MB |
LG CED-8042 | CD-RW | 610 MB |
Memorex CDRW-4420s | CD-RW | 610 MB |
Mitsubishi CDRW226 | CD-RW | 610 MB | Requires firmware version 1.20.
Mitsubishi CDRW4420 | CD-RW | 610 MB |
Mitsumi CR-2802TE | CD-RW | 610 MB |
Mitsumi CR-4802TE | CD-RW | 610 MB |
Mitsumi CR-4804TE | CD-RW | 610 MB |
Olympus CDS-615E, -620E, -630E | CD-R | 610 MB |
Optima CD-R 650, 1300 | CD-R | 610 MB |
Panasonic CW-7502 | CD-R | 610 MB |
Panasonic CW-7582 | CD-R | 610 MB |
Philips OmniWriter 26 | CD-RW | 610 MB | Requires firmware version 1.20.
Philips 3600 | CD-RW | 610 MB |
Philips CDD3610 | CD-RW | 610 MB |
Philips CDD3801 | CD-RW | 610 MB |
Philips PCA382RW | CD-RW | 610 MB |
Philips CDD4201 | CD-RW | 610 MB |
Plextor PlexWriter PX-R412 | CD-R | 610 MB |
Plextor PlexWriter RW PX-R4220T | CD-RW | 610 MB |
Plextor PlexWriter PX-R820T | CD-R | 610 MB |
Plextor PlexWriter RW PX-W8220T | CD-RW | 610 MB |
Plextor PX-W124T | CD-RW | 610 MB |
Plextor PX-W8432T | CD-RW | 610 MB |
Ricoh MP6200S, MP6201S | CD-RW | 610 MB | Requires firmware version 1.20.
Ricoh MP6211S | CD-RW | 610 MB | Requires firmware version 1.20.
Ricoh MP7040S | CD-RW | 610 MB |
Ricoh MP7040A | CD-RW | 610 MB | Requires firmware version 1.30.
Ricoh MP7060A | CD-RW | 610 MB |
Ricoh 7080A | CD-RW | 610 MB |
Ricoh DVD/CD-RW 9060A | CD-RW/DVD-ROM | 610 MB |
Smart and Friendly CD-R1002 | CD-R | 610 MB |
Smart and Friendly CD-R2004 | CD-R | 610 MB |
Smart and Friendly CD-R2006 | CD-R | 610 MB | Requires firmware version 1.1e.
Smart and Friendly CD-R4006 | CD-R | 610 MB | Requires firmware version 1.0j.
Smart and Friendly CD-RW 426 | CD-RW | 610 MB | Requires firmware version 1.0g.
Smart and Friendly CD SpeedRacer | CD-RW | 610 MB |
Smart and Friendly CD TurboWriter | CD-R | 610 MB |
Smart and Friendly CD-RW6424A | CD-RW | 610 MB |
Smart and Friendly CD-RW6424S | CD-RW | 610 MB |
Sony CDU920, -924, -926, -948 | CD-R | 610 MB | Model 926 requires firmware version 1.1e.
Sony CRX100E | CD-RW | 610 MB |
Sony CRX100E/X | CD-RW | 610 MB | Supported under Windows 98 only.
Sony CRX100E/X2 | CD-RW | 610 MB | Supported under Windows 98 and 2000 only.
Sony CRX120E | CD-RW | 610 MB |
Sony CRX120Eu | CD-RW | 610 MB | Supported under Windows 98 and 2000 only.
Sony CRX120Ei-DV | CD-RW | 610 MB | Supported under Windows 98 and 2000 only.
Sony CRX120E/X | CD-RW | 610 MB | Supported under Windows 98 and 2000 only.
Sony CRX140E | CD-RW | 610 MB |
Sony CRX140S | CD-RW | 610 MB |
Sony CRX145E | CD-RW | 610 MB |
Sony CRX145E/X | CD-RW | 610 MB | Supported under Windows 98 and 2000 only.
Sony CRX145S | CD-RW | 610 MB |
TEAC CD-R56S | CD-R | 610 MB |
TEAC CD-R56S-4 | CD-R | 610 MB |
TEAC CD-R58S | CD-R | 610 MB |
Traxdata SCSI-CD ReWritable-2x2x6, CRW2260 Pro | CD-RW | 610 MB |
Traxdata CD-RW2260 Pro, CDRW4260 Pro | CD-RW | 610 MB | Requires firmware version 1.0g.
Traxdata CD-RW2224 Plus | CD-RW | 610 MB |
Waitec WT2036 | CD-RW | 610 MB |
Waitec WT4046 | CD-RW | 610 MB |
Waitec WT2444 | CD-RW | 610 MB |
Waitec WT2422 | CD-RW | 610 MB |
Yamaha CDR400c, CDR200c | CD-R | 610 MB | Requires firmware version 1.0j.
Yamaha 2260, 4260 | CD-RW | 610 MB | Requires firmware version 1.0g.
Yamaha 2216, 4416 | CD-RW | 610 MB |
Yamaha CDR401t | CD-RW | 610 MB |
Yamaha CRW4001 | CD-RW | 610 MB |
Yamaha CRW4261 | CD-RW | 610 MB |
Yamaha CRW2216E | CD-RW | 610 MB |
Yamaha CRW4416E | CD-RW | 610 MB |
Yamaha CRW6416E | CD-RW | 610 MB |
Yamaha CRW6416S | CD-RW | 610 MB |
Yamaha CRW8424S | CD-RW | 610 MB |

Ricoh drives:
  Ricoh recommends you use media from the following manufacturers only: Ricoh, Kao, Taiyo Yuden, Mitsui Toatsu, TDK, and Kodak.

Yamaha drives:
  To update your drive's firmware, visit Yamaha's web site.

### Tape Drives

Retrospect is all the software required to support most tape drives.

- DAT Drives
- ADR Drives
- 8mm Drives
- AIT and AME Drives
- DLT(tm) Drives
- DTF Drives
- Travan Drives
- DC6000 Drives
- DC2000 Drives

NOTE: Regular cleaning of your tape drive is essential for reliable performance. Dirty drive heads are the number one cause of tape drive problems and reported media failures (error -206). Retrospect can remind you to clean your drive at the specified interval of hours of tape drive use. See the Retrospect User's Guide. Refer to your drive's documentation for its manufacturer's cleaning recommendations.

NOTE: If you wish to exchange tapes with people who do not have compression drives, turn off Retrospect's hardware compression option when creating backup sets.

#### DAT Drives

DAT cartridges are available in lengths of 60 to 150 meters and range in capacity from 1.2 GB to 20 GB.

The following table shows the different tape lengths supported by the different DDS formats. It also shows the uncompressed capacity of each tape length when used on a drive of a given format.

DAT Format and Tape Length Capacity and Compatibility
| 60m | 90m | 120m | 125m | 150m
--- | --- | --- | --- | --- | ---
DDS | 1.2 GB | 1.9 GB | not supported | not supported | not supported
DDS-2 | 1.2 GB | 1.9 GB | 4 GB | not supported | not supported
DDS-3 | 1.2 GB | 1.9 GB | 4 GB | 12 GB | not supported
DDS-4 | 1.2 GB | 1.9 GB | 4 GB | 12 GB | 20 GB

Tapes created on one drive can typically--but not always--be read by drives of another manufacturer, provided they are of the same format. A few drives use the DataDAT and DVDS formats, neither of which is compatible with the more common DDS format or its successors. Use care when interchanging tapes among drives from different vendors: DAT tapes written in one drive may erroneously show as "erased" when inserted in a DAT drive using a mechanism from a different manufacturer. During unattended backup, Retrospect automatically overwrites tapes that appear as erased.

Though they are derived from the same technology and use the acronym for Digital Audio Tape, DAT drives should be used with only data grade tapes--not audio grade--for reliable storage.

Older data grade DAT tapes may not implement the Media Recognition System, required for use by some DAT drives. Problems with non-MRS data grade tapes (for example, the tapes appear as write-locked) are best solved by using MRS tapes, recognizable by the MRS logo on their packaging. Should you insist on using non-MRS tapes, contact the drive vendor for assistance. (Some drives' MRS requirements can be turned off with a DIP switch.)

Supported DAT Mechanisms
Mechanism | Format | Maximum tape length | Hardware compression | Comments
--- | --- | --- | --- | ---
AIWA GD-8000 | DDS-2 | 120m | Yes |
Archive/Conner Python | DDS | 90m | Optional | See firmware notes below.
Archive/Conner Turbo Python | DDS | 90m | Yes | See firmware notes below.
Compaq 2/4 GB DAT | DDS | 90m | Yes |
Compaq 2/8 GB DAT | DDS | 90m | Yes |
Compaq 4/8 GB DAT | DDS-2 | 120m | Yes |
Compaq 4/16 GB Turbo DAT | DDS-2 | 120m | Yes |
Compaq 12/24 GB DAT | DDS-3 | 125m | Yes |
Compaq 20/40 GB DAT | DDS-4 | 150m | Yes |
Conner/Seagate CTD-2004 | DDS | 90m | Optional |
Conner/Seagate CTD-4004 | DDS | 90m | Yes |
Conner/Seagate CTD-8000 | DDS-2 | 120m | Yes |
Conner/Seagate CTD-8005 | DDS-2 | 120m | Yes |
Cybernetics CY-1000 | DDS-2 | 120m | Yes | Only stock configuration supported.
Cybernetics CY-1200 | DDS-3 | 125m | Yes | Only stock configuration supported
Dell PowerVault 100T DDS-3 | DDS-3 | 125m | Yes |
Dell PowerVault 100T DDS4 | DDS-4 | 150m | Yes |
HP 35450A | DDS | 60m | No |
HP 35470A, C1534A | DDS | 90m | No |
HP 35480A, C1536A | DDS | 90m | Yes |
HP C1533A, C1539A | DDS-2 | 120m | Yes |
HP C1537A | DDS-3 | 125m | Yes |
HP C5683A | DDS-4 | 150m | Yes |
IBM DDS-4 00N7991 | DDS-4 | 150m | Yes |
Indigita iDT-2500 | DVDS or DDS | 120m | No | DVDS format is incompatible with DDS formats.
Indigita iDT-2700 | DVDS or DDS | 120m | Yes | DVDS format is incompatible with DDS formats.
Indigita iDT-2900 | DVDS or DDS-2 | 120m | Yes | DVDS format is incompatible with DDS formats.
Maxoptix MaxDAT | DDS-3 | 125m | Yes |
MKE LKM-DB1E | DDS-3 | 125m | Yes |
Seagate STD 12000 | DDS | 90m | No |
Seagate STD 14000 | DDS | 90m | Yes |
Seagate STD 28000 | DDS-2 | 120m | Yes |
Seagate STD 124000 | DDS-3 | 125m | Yes |
Seagate Scorpion 40 | DDS-4 | 150m | Yes |
Sony SDT-2000, -2000E | DDS | 90m | No | Model 2000E is double-speed.
Sony SDT-4000, -4000E | DDS | 90m | Yes | Model 4000E is double-speed.
Sony SDT-5000, -7000 | DDS-2 | 120m | Yes | Model 7000 is quad-speed.
Sony SDT-5200, -7200 | DDS-2 | 120m | No |
Sony SDT-9000 | DDS-3 | 125m | Yes |
Sony SDT-10000 | DDS-4 | 150m | Yes |
WangDAT 3100 | DDS | 90m | No |
WangDAT 3200 | DDS | 90m | Yes |
WangDAT 3300 | DDS-2 | 120m | No |
WangDAT 3400 | DDS-2 | 120m | Yes |
WangDAT 3800 | DDS-2 | 120m | Yes |
WangDAT 3900 | DDS-3 | 125m | Yes |

Archive/Conner Python (non-compression):
  Make sure you have firmware version 2.39 or later; version 2.26 will not function properly. Determine your firmware version by clicking Retrospect's Device Status button. To upgrade, contact your drive vendor or call Conner/Seagate at 800.732.4283. Outside the U.S., to find your local customer service office, visit Seagate's web site.

Archive/Conner Python Turbo:
  Make sure you have firmware version 4.08 or later; version 4.04 will not function properly. Determine your firmware version by clicking Retrospect's Device Status button. To upgrade, contact your drive vendor or call Conner/Seagate at 800.732.4283. Outside the U.S., to find your local customer service office, visit Seagate's web site.

Cybernetics:
  Stock configuration includes backlit status display but does not include Cybernetics data compression, advanced SCSI processor, Cybernetics data encryption, accelerated file access, robotic control software, or high speed tape cache.

#### ADR Drives

Supported ADR drives can store up to 25 GB of uncompressed data on a tape cartridge.

Supported ADR Mechanisms
Mechanism | Capacity | Cartridges | Hardware compression | Comments
--- | --- | --- | --- | ---
OnStream Echo SC30, DI30 | 15 GB | ADR30 | No | Requires firmware version 1.06. See model DI30 notes below.
OnStream Echo SC50 | 25 GB | ADR50 | No | Requires firmware version 1.06.
OnStream ADR50 | 25 GB | ADR50 | Yes | Cannot read tapes written by Echo 30 or 50.

OnStream Echo 30 and 50:
  To update your drive's firmware, visit OnStream's web site.

OnStream Echo DI30:
  With this IDE/ATAPI interface model, pressing the drive's eject button while it is writing causes Retrospect to report error -204 (device busy) before ejecting the tape. This is caused by a bug in the drive's firmware, which has been reported to OnStream. To avoid this error, stop the backup in Retrospect before pressing the drive's eject button.

#### 8mm Drives

When an 8mm drive is turned on, it automatically sets itself to the highest capacity possible for that drive. When a new tape is inserted and erased by Retrospect, it is initialized to the drive's current setting. Once initialized, the tape retains its density/compression setting. If you own only one kind of Exabyte drive and buy new tapes, maximum capacity will be achieved by default. You can format tapes in your choice of density format by inserting a tape in the drive, going to Configure>Devices, selecting the tape, and choosing Format from the devices toolbar. After confirming the format, Retrospect asks you which drive density format to use.

Supported 8mm Mechanisms
Mechanism | Capacity | Hardware compression | Comments
--- | --- | --- | ---
Cybernetics CY-8705 | 7 GB | Yes | Only stock configuration supported.
Exabyte EXB-8200, -8200SX | 2 GB | No | Retrospect does not use the high speed search of model 8200SX.
Exabyte EXB-8205 | 2 GB | Yes |
Exabyte EXB-8205XL | 3.5 GB | Yes |
Exabyte EXB-8500 | 5 GB | No |
Exabyte EXB-8500c, -8505 | 5 GB | Yes |
Exabyte EXB-8505XL, -8700, -8700LT, -8700SW, Eliant 820 | 7 GB | Yes |

Cybernetics:
  Stock configuration includes backlit status display but does not include Cybernetics data compression, advanced SCSI processor, Cybernetics data encryption, accelerated file access, robotic control software, or high speed tape cache.

#### AIT and AME Drives

Drives of a given capacity are compatible with one another but not with drives of other capacities.

Supported AIT and AME Mechanisms
Mechanism | Capacity | Hardware compression | Comments
--- | --- | --- | ---
ADIC AIT 70D | 35 GB | Yes |
ADIC AIT 100D | 50 GB | Yes |
Compaq AIT 35 GB | 35 GB | Yes |
Compaq AIT 50 GB | 50 GB | Yes |
Cybernetics CY-8000 | 25, 35 GB | Yes | Only stock configuration supported. Requires firmware version 0400 or later to use 35 GB tapes.
Cybernetics CY-8050 | 50 GB | Yes | Only stock configuration supported.
Cybernetics CY-8900 | 20 GB | Yes | Only stock configuration supported.
Ecrix VXA-1 | 12, 33 GB | Yes |
Exabyte EXB-8900 | 20 GB | Yes |
Exabyte Mammoth LT | 14 GB | Yes |
Exabyte Mammoth 2 | 60 GB | Yes |
Seagate Sidewinder 50 | 25, 35 GB | Yes | Requires firmware version 0400 or later to use 35 GB tapes.
Sony SDX-300 | 25 GB | No |
Sony SDX-300c | 25, 35 GB | Yes | Requires firmware version 0400 or later to use 35 GB tapes.
Sony SDX-500 | 50 GB | Yes |

Cybernetics:
  Stock configuration includes backlit status display but does not include Cybernetics data compression, advanced SCSI processor, Cybernetics data encryption, accelerated file access, robotic control software, or high speed tape cache.

#### DLT(tm) Drives

Supported DLT Mechanisms
Mechanism | Capacity | Cartridges | Hardware compression | Comments
--- | --- | --- | --- | ---
ADIC DS9400D/L | 20 GB | CT III and IV | Yes |
ADIC DS9700 | 35 GB | all CompacTape | Yes |
ADIC DS9800 | 40 GB | all CompacTape | Yes |
Compaq 10/20 GB DLT | 10 GB | CT III | Yes |
Compaq 15/30 GB DLT | 15 GB | CT III and IIIXT | Yes |
Compaq 20/40 GB DLT | 20 GB | CT III and IV | Yes |
Compaq 35/70 GB DLT | 35 GB | all CompacTape | Yes |
Cybernetics CY-4000 | 20 GB | CT III and IV | Yes | Only stock configuration supported.
Cybernetics CY-4700 | 35 GB | All CompacTape | Yes | Only stock configuration supported.
DEC THZ01 | 2.6 GB | CT III | No |
DEC THZ02 | 6 GB | CT III | No |
DEC DLT-2000 | 10 GB | CT III | Yes |
Dell PowerVault 110 DLT4 | 20 GB | CT III and IV | Yes |
Dell PowerVault 110 DLT7 | 35 GB | All CompacTape | Yes |
Dell PowerVault 110 DLT8 | 40 GB | all CompacTape | Yes |
HP C1549A | 15 GB | CT III and IIIXT | Yes |
HP C1579A | 20 GB | CT III and IV | Yes |
HP C5658A | 35 GB | all CompacTape | Yes |
Quantum THZ01 | 2.6 GB | CT III | No |
Quantum THZ02 | 6 GB | CT III | No |
Quantum DLT2000 | 10 GB | CT III | Yes |
Quantum DLT2000XT | 15 GB | CT III and IIIXT | Yes |
Quantum DLT4000 | 20 GB | CT III and IV | Yes |
Quantum DLT7000 | 35 GB | all CompacTape | Yes |
Quantum DLT8000 | 40 GB | all CompacTape | Yes |
Tandberg DLT4000 | 20 GB | CT III and IV | Yes |
Tandberg DLT7000 | 35 GB | all CompacTape | Yes |
Tandberg DLT8000 | 40 GB | all CompacTape | Yes |

Cybernetics:
  Stock configuration includes backlit status display but does not include Cybernetics data compression, advanced SCSI processor, Cybernetics data encryption, accelerated file access, robotic control software, or high speed tape cache.

#### DTF Drives

Supported DTF Mechanisms
Mechanism | Capacity | Cartridges | Hardware compression | Comments
--- | --- | --- | --- | ---
Cybernetics CY-9000LP | 12 or 42 GB | GW-240S or GW-730L | Yes | Only stock configuration supported.
Sony GY-2120 | 12 or 42 GB | GW-240S or GW-730L | Yes |

Cybernetics:
  Stock configuration includes backlit status display but does not include Cybernetics data compression, advanced SCSI processor, Cybernetics data encryption, accelerated file access, robotic control software, or high speed tape cache.

#### Travan Drives

For best results with Travan drives, rewind tapes before you eject them. To remove a tape from a drive, first click the Eject button in the storage devices window or quit Retrospect (which automatically rewinds tapes). Then wait while the drive rewinds the tape. When the access stops, you may remove the tape.

Travan TR-5 and NS20 drives can write only to TR-5 tape cartridges, but they can read QIC-3095 and TR-4 tapes.

Supported Travan Mechanisms
Mechanism | Capacity | Cartridges | Hardware compression | Comments
--- | --- | --- | --- | ---
AIWA NS20 | 10 GB | TR-5 | Yes | See note below.
AIWA TD-8000 | 2 or 4 GB | QIC-3095 or TR-4 | No |
AIWA TD-8001 | 2 or 4 GB | QIC-3095 or TR-4 | Yes |
AIWA TD-A8000 | 2 or 4 GB | QIC-3095 or TR-4 | No |
Conner/Seagate CTT-8000 | 1.5, 2.0, or 4 GB | QIC-3095 or TR-4 | No |
Conner/Seagate CTT-8000A | 2 or 4 GB | QIC-3095 or TR-4 | No |
Exabyte Eagle NS8 | 2 or 4 GB | QIC-3095 or TR-4 | Optional |
HP Colorado 5 GB | 2.5 GB | QIC-3095 or HP Colorado 5 GB | No |
HP Colorado 8 GB | 4 GB | QIC-3095, TR-4, or HP Colorado 5 GB | No |
HP Colorado 14 GB | 7 GB | HP Colorado 14 GB | No |
HP Colorado 20 GB | 10 GB | TR-5, HP Colorado 14 GB | No |
HP SureStore T4 | 4 GB | QIC-3095 or TR-4 | No |
HP SureStore T20 | 10 GB | TR-5 | No |
Seagate NS20 | 10 GB | TR-5 | Yes | See note below.
Seagate TR-5 | 10 GB | TR-5 | No | See note below.
Seagate STT-8000N, Hornet 8 | 1.5, 2.0, or 4 GB | QIC-3095 or TR-4 | Optional |
Seagate STT-8000A | 4 GB | QIC-3095 or TR-4 | No |
Seagate STT-20000A | 10 GB | TR-5 | No |
Tandberg NS20 | 10 GB | TR-5 | Yes | See note below.
Tandberg NS8 | 2 or 4 GB | QIC-3095 or TR-4 | Yes |
Tandberg TR4 | 2 or 4 GB | QIC-3095 or TR-4 | No |
Tecmar NS20 | 10 GB | TR-5 | Yes |
Tecmar NS8 | 2 or 4 GB | QIC-3095 or TR-4 | Yes |
Tecmar NS20 ATAPI | 10 GB | TR-5 | Yes |
Wangtek TS-420c | 2 or 4 GB | QIC-3095 or TR-4 | Yes |

AIWA NS20:
  If you remove the tape from the drive before it is rewound or the computer crashes before Retrospect rewinds the tape for its verification pass, the tape cannot be appended to. This may be remedied by a future firmware revision. Contact AIWA (888.297.3004 in U.S.).

Seagate and Tandberg NS20 and TR-5:
  If you remove the tape from the drive before it is rewound or the computer crashes before Retrospect rewinds the tape for its verification pass, the tape cannot be appended to and the drive will hang the computer on any attempt to append to such a tape. This may be remedied by a future firmware revision. Contact your drive vendor: Conner/Seagate (800.732.4283 in U.S.), or Tandberg (805.579.1000 in U.S.).

#### DC6000 Drives

Tapes written by one drive can typically be read by another of equal or greater capacity.

A separate formatting step is not required, though the first time Retrospect uses a DC6000 tape, it performs a "long erase," which retensions the tape, erases all previous data, and determines the tape's format and capacity.

Supported DC6000 Mechanisms
Mechanism | Capacity | Hardware compression | Comments
--- | --- | --- | ---
Compaq SLR | 150, 250, 320, 525, 1000, 1200, 2000, 2500 MB, 4 GB | Yes, special | Hardware compression is available only with DC9200, DC9250, and SLR5 media.
Tandberg SLR1 (3600) | 120, 150, 250 MB | No |
Tandberg SLR2 (3800) | 120, 150, 250, 320, 525 MB | No |
Tandberg SLR3 (4100) | 120, 150, 250, 320, 525, 1000 MB | No |
Tandberg SLR4 (4200) | 120, 150, 250, 320, 525, 1000, 2000 MB | No | When performing network backups enable the Retension tapes option in Special>Preferences>Media>Handling.
Tandberg SLR4DC (4222) | 120, 150, 250, 320, 525, 1000, 2000, 2500 MB | Optional | Hardware compression is available. When performing network backups enable the Retension tapes option in Special>Preferences>Media>Handling.
Tandberg SLR5 | 150, 250, 320, 525, 1000, 1200, 2000, 2500 MB, 4 GB | Yes, special | Hardware compression is available only with DC9200, DC9250, and SLR5 media.
Tandberg SLR24 (SLR6) | 12 GB | Yes | Writes only to 12 GB SLR6 media but reads other DC6000 media.
Tandberg SLR32 (MLR1) | 13, 16 GB | Yes | Uses MLR1 cartridges and can read and write other DC6000 QIC cartridges.
Tandberg SLR50 (MLR3) | 25 GB | Yes | Uses SLR5, MLR1, or MLR3 cartridges and can read other DC6000 QIC cartridges.
Tandberg SLR100 | 50 GB | Yes | Uses SLR100 and SLR50 cartridges and can read SLR24 and SLR32 cartridges.
Wangtek 51000 | 120, 150, 250, 320, 525, 1000 MB | No | When performing network backups enable the Retension tapes option in Special>Preferences>Media>Handling.
Wangtek 9500 | 120, 150, 250, 320, 525, 1000, 1350, 2100, 2500, 5000 MB | No | When performing network backups enable the Retension tapes option in Special>Preferences>Media>Handling.
Wangtek 9500DC | 120, 150, 250, 320, 525, 1000, 1350, 2100, 2500, 5000 MB | Yes | When performing network backups enable the Retension tapes option in Special>Preferences>Media>Handling.

#### DC2000 Drives

Streaming, or sequential mode, DC2000 drives are similar to DC6000 drives in that they are not block-addressable, and some of these do not require time-consuming formatting. For best results with DC2000 sequential mode drives, rewind tapes before you eject them. To remove a tape from a drive, first click the Eject toolbar icon in the storage devices window or quit Retrospect. Then wait while the drive rewinds the tape. When the access stops, you may remove the tape.

Supported DC2000 Sequential Mode Mechanisms
Mechanism | Capacity | Cartridges | Hardware compression | Comments
--- | --- | --- | --- | ---
Tandberg Panther Mini 2000 (TDC-3500) | 750, 840, 1000 MB | MC3000, MC3000XL, or QW3000XL | No |
Tandberg Panther Mini 4600 (TDC-3700) | 750, 840, 1000, 2300 MB | MC3000, MC3000XL, QW3000XL, or QWX3210XL | No |

### Libraries

Libraries with nine or more tape slots require Retrospect Workgroup Backup or Retrospect Server Backup. Retrospect Desktop Backup supports libraries with up to eight tape slots.

Some libraries have the tape drive at one SCSI address and the loading mechanism at another, whereas others integrate the two into a single SCSI address. Retrospect uses only one drive at a time with loaders having two or more drives. Refer to the Retrospect User's Guide for information on Retrospect's library features.

Choose Eject Magazine from the devices toolbar to clear the tape drive or drives before opening the door or removing the tape magazine.

Some libraries have LCD panels to control actions such as ejecting tapes from drives and moving tapes between slots. Retrospect can encounter problems when you use the LCD controls to manipulate the library while Retrospect is also manipulating the library. Avoid trouble by controlling library functions only from Retrospect, or exit Retrospect before you use the library's manual controls.

Retrospect supports designating a slot in a library exclusively for a cleaning cartridge. With a slot designated for a cleaning cartridge, Retrospect will not move a tape from that slot to the drive when Retrospect scans slots to find a tape. To clean the library's tape drive, use the library's controls to move the cleaning cartridge from its slot to the tape drive. Refer to your library's documentation for its manufacturer's cleaning recommendations. If you put a cleaning cartridge in a library slot, be sure to designate that slot as reserved by selecting the slot in Retrospect's devices window and choosing Cleaning Slot from the toolbar.

Supported Libraries
Library | Mechanism | Cartridge Slots | SCSI ID Addressing (Robotics/Drive) | Comments
--- | --- | --- | --- | ---
ADIC 1200 | HP 35480A, Sony SDT-5000, or WangDAT 3400 | 12 | Separate, special | The drive's ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively. See notes below.
ADIC FastStor DLT | Quantum DLT | 7 | Separate |
ADIC FastStor 22 | Quantum DLT | 22 | Separate |
ADIC QLS 4G series | one to four DDS-3 DAT | 36, 72, or 144 | Separate |
ADIC QLS SDX series | two to six Sony AIT | 20, 40, 60, 80, or 120 | Separate |
ADIC Scalar 218 series | one or two Quantum DLT | 18 | Separate |
ADIC Scalar 220 series | one or two Sony AIT | 20 | Separate |
ADIC Scalar 224/448/458 series | two or four Quantum DLT | 24 or 48 | Separate |
ADIC Scalar 480 series | two to four Sony AIT | 80 | Separate |
ADIC VLS 4mm series | one or two Sony SDT-5000 | 15 | Separate | See notes below.
ADIC VLS 8mm series | one or two Exabyte EXB-8205, -8205XL, -8505, or -8505XL | 15 | Separate | See notes below.
ADIC VLS SDX series | one or two Sony AIT | 11 | Separate | See notes below.
ADIC VLS DLT series | Quantum DLT | 7 | Separate | See notes below.
ATL PowerStor L200 series | Quantum DLT | 8 | Separate |
ATL PowerStor L500 series | one to three Quantum DLT | 14 | Separate |
AIWA AL-17D/210/220 | one or two Sony SDT-5000 | 17 | Separate |
AIWA AL-D310 | Sony SDT-9000 | 17 | Separate |
Archive/Conner Python | Python | 5 or 12 | Integrated |
Archive/Conner DiamondBack | Turbo Python | 4 or 12 | Integrated |
Box Hill Shadow Box | Quantum DLT | 15 | Separate |
Box Hill DLT Seven Box | Quantum DLT | 7 | Integrated |
Box Hill DLT Five Box | Quantum DLT | 5 | Integrated |
Box Hill Borg Box series | two or four Exabyte Eliant 820 or EXB-8900 | 40 or 80 | Separate |
Box Hill Light Box series | one or two Exabyte Eliant 820 or EXB-8900 | 11 or 21 | Separate |
Box Hill Bread Box | Exabyte Eliant 820 | 10 | Separate, special | The drive's ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively.
Breece Hill Q2/15 | one or two DLT | 15 | Separate |
Breece Hill Q7 | one or two DLT | 28 | Separate |
Compaq 12/24 GB DAT 8 Cassette Autoloader | 12/24 GB DAT | 8 | Integrated |
Compaq DLT 20/40 Mini-Library | one or two 20/40 GB DLT | 15 | Separate |
Compaq DLT 35/70 Mini-Library | one or two 35/70 GB DLT | 15 | Separate |
Compaq TL881 DLT Mini-Library series | one or two 20/40 GB DLT | 10 or 26 | Separate |
Compaq TL891 DLT Mini-Library series | one or two 35/70 GB DLT | 10 or 26 | Separate |
Compaq TL895 DLT Library | two to seven 35/70 GB DLT | 96 | Separate |
Cybernetics CY-TL1-1008, -2018, -2036, -4036, -4072, -4144 | one to four CY-1200 | 8, 18, 36, 72, 144 | Separate | Only stock configuration supported.
Cybernetics CY-TL4-1010, -2010, -2020, -4030, -4060 | one to four CY-4000 or -4700 | 10, 20, 30, 60 | Separate | Only stock configuration supported.
Cybernetics CY-TL8-1004 | CY-8000 | 4 | Integrated | Only stock configuration supported. See note below.
Cybernetics CY-TL8-1007 | CY-8900 | 7 | Separate | Only stock configuration supported. See note below.
Cybernetics CY-TL8-2010, -2020, -4020, -4040, -4080, -6060, -6120 | one to six CY-8000, -8050, -8900, or -8705 | 10, 20, 40, 60, 80, 120 | Separate | Only stock configuration supported.
Cybernetics CY-TL8-2015, 2030 | one or two CY-8000 or -8050 | 15 or 30 | Separate | Only stock configuration supported.
Cybernetics CY-TL9-1009 | CY-9000LP | 8 | Separate | Only stock configuration supported.
Dell PowerVault 120T DDS Autoloader series | PowerVault 100T DDS3 or DDS4 | 8 | Integrated |
Dell PowerVault 120T DLT Autoloader | PowerVault 110T DLT4, DLT7, or DLT8 | 7 | Separate |
Dell PowerVault 130T DLT Tape Library | one to four PowerVault 110T DLT4, DLT7, or DLT8 | 30 | Separate |
Exabyte 10i, 10e, 10h | EXB-8200, -8200SX, -8500, or -8500C | 10 | Separate, special | The drive's ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively.
Exabyte 17D | DLT | 7 | Separate |
Exabyte EZ 17 | EXB-8900 | 7 | Separate | See note below.
Exabyte 18D | Quantum DLT | 7 | Separate |
Exabyte 210 | one or two EXB-8205 or -8505 | 11 | Separate |
Exabyte 218 | one or two DAT drives | 18 | Separate |
Exabyte 220 | one or two EXB-8900 or Eliant 820 | 20 | Separate |
Exabyte 230D | one or two Quantum DLT | 30 | Separate |
Exabyte 440/480 | one to four Eliant 820 or EXB-8900 | 40 or 80 | Separate |
Exabyte 690D | two to six DLT | 30, 60, 90 | Separate |
Exabyte X200 | two to ten EXB-8900 | 40, 80, 120 | Separate | Configurations with 160 or 200 slots are not supported.
HP C1553A | C1533A | 6 | Integrated |
HP C1557A | C1537A | 6 | Integrated |
HP SureStore DLT 15 series | one or two Quantum DLT | 15 | Separate |
HP SureStore DLT 28/48 series | one or two Quantum DLT | 28 or 48 | Separate |
HP SureStore DLT 418 | Quantum DLT | 8 | Separate |
HP C5713A DAT 40x6 | C5683A DAT40 | 6 | Integrated |
Imation ITL 1000 series | two or four Tandberg MLR1 or MLR3 | 10, 20, or 40 | Separate |
Imation ITL DLT 115 series | Quantum DLT | 14 | Separate |
Imation ITL 4000 series | one or two Travan NS8 or NS20 | 15 | Separate |
Imation ITL 2225 | one or two DDS-2 DAT | 25 | Separate, special | If only one drive its ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively. The second drive ID must be one higher than the first drive.
Imation ITL 3225 | one or two DDS-3 DAT | 25 | Separate, special | If only one drive its ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively. The second drive ID must be one higher than the first drive.
LAGO LS-340L | one or two HP C1533A | 25 | Separate, special | If only one drive its ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively. The second drive ID must be one higher than the first drive.
Overland Data LoaderXpress series | Quantum DLT | 5 or 10 | Separate |
Overland Data LXS MiniLibrary series | Quantum DLT | 15 | Separate |
Overland Data LibraryXpress LXB series | one or two Quantum DLT | 10 | Separate |
Overland Data LibraryXpress system series | two to eight Quantum DLT | 26, 36, 42, 52, or 120 | Separate |
Qualstar TLS-2000 | one to four DDS-2 or DDS-3 DAT | 18, 36, 72, or 144 | Separate |
Qualstar TLS-4000 series | one to six Exabyte EXB-8205, -8505, -8505XL or Sony AIT | 10, 20, 40, 60, 80, or 120 | Separate |
Qualstar TLS-6000 series | one to four Quantum DLT | 10, 20, 30, or 60 | Separate |
Quantum DLT 2500, 2500XT, 4500 | DLT | 5 | Integrated | See notes below.
Quantum DLT 2700, 2700XT, 4700 | DLT | 7 | Integrated | See notes below.
Quantum DLTstor 108 series | DLT | 8 | Separate |
Quantum DLTstor 114 series | DLT | 14 | Integrated | See note below.
Quantum PowerStor L200 series | DLT | 8 | Separate |
Quantum PowerStor L500 series | one to three DLT | 14 | Separate |
Seagate Scorpion 96 | STD 124000 | 4 | Integrated |
Seagate Sidewinder 200 | Sidewinder 50 | 4 | Integrated | See note below.
Seagate DDS-4 Autoloader | Scorpion 40 | 6 | Integrated |
Sony DMS-B9 | GY-2120 | 9 | Separate |
Sony TSL-A300c | SDX-300c | 4 | Integrated | See note below.
Sony TSL-7000, 9000 | SDT-7000, -9000 | 8 | Integrated |
Sony TSL-11000 | SDT-10000 | 8 | Integrated |
Spectra Logic Spectra 215 | one or two Travan NS8 or NS20 | 15 | Separate |
Spectra Logic Spectra 2000 | one or two Sony AIT | 15 or 30 | Separate |
Spectra Logic Spectra 4000 | one to four HP C1533A | 20, 40, 60 | Separate |
Spectra Logic Spectra 5000 | one to four Sony SDT-9000 | 20, 40, or 60 | Separate |
Spectra Logic Spectra 10000 | one to four Sony AIT | 20 or 40 | Separate |
StorageTek 9724 | one or two DDS-2 DAT | 25 | Separate, special | If only one drive its ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively. The second drive ID must be one higher than the first drive.
StorageTek 9734 | one or two DDS-3 DAT | 25 | Separate, special | If only one drive its ID must be set to 0, 1, 2, or 3, and the loader's address must be three higher, at 3, 4, 5, or 6 respectively. The second drive ID must be one higher than the first drive.
Straightline SL800 series | one to four Exabyte EXB-8900 or one to five Sony AIT | 10 to 150, in increments of 10 | Separate |
Tandberg MLR library series | two or four MLR1 or MLR3 | 10, 20, or 40 | Separate |
Tandberg SLR Autoloader | SLR | 8 | Separate |
Tecmar LD8 | WangDAT 3800 or 3900 | 8 | Integrated |

ADIC 1200 series:
  After ejecting the magazine with the devices toolbar, press the Unload button on the loader before opening the door. After reloading close the door and press the Load button. The ADIC loader firmware must be version 0458 or greater or the loader mechanism will not be seen by Retrospect. Each time you restart your computer, you must unload and load the ADIC 1200 library.

ADIC VLS series:
  Changing the Magazine: After ejecting the magazine with the devices toolbar, quit Retrospect. Press the Alt button on the loader then press the Down/Unload button. When the loader has positioned itself in the "unload" state open the door and remove the magazine. After adding, removing, or replacing tapes in the magazine, load the magazine and close the door. Press the Alt button then press the Up/Load button. Wait until the loader is fully initialized before starting Retrospect.

Cybernetics:
  Stock configuration includes backlit status display but does not include Cybernetics data compression, advanced SCSI processor, Cybernetics data encryption, accelerated file access, robotic control software, or high speed tape cache.

Exabyte EZ 17, Cybernetics CY-TL8-1007:
  Unload any tape cartridge in the drive when you power on the loader or when you change its magazines. This allows it to properly report the slot positions of tapes to Retrospect.

Quantum DLTstor 114 series:
  A Quantum DLTstor 114 has three modes which are set using the operator control panel on the front of the loader. The modes are Normal, Density Select, and Maintenance. To work with Retrospect, the library must be in Normal mode.

  Changing the Magazine when Retrospect is Open: To change tapes in a magazine, first choose Eject Magazine from Retrospect's devices toolbar. Press the loader's Open button and pull open the door. Load the magazine completely with your desired tapes, replace the magazine in the loader, and push the door closed. Press the Load/Unload button to move the first tape from the magazine to the drive.

  Changing the Magazine when Retrospect is Not Open: To change the magazine when Retrospect is not open you need not take any special action.

  Tape Slot Numbers: Each magazine has seven slots numbered 0 through 6; ignore these numbers. Consider the magazine slots numbered 1 through 14 from left to right, corresponding to Retrospect's slot numbers.

Quantum DLT2500 through -4500 series:
  Changing the Magazine when Retrospect is Open: To eject the magazine, first choose Eject Magazine from Retrospect's devices toolbar. Turn the loader's key to the unlocked position and press the Open button. When the sliding door opens, pull out the magazine. Load the magazine completely with your desired tapes, replace the magazine in the loader, then slide the door closed. Press the library's Load button to move the first tape from the magazine into the drive.

  Changing the Magazine when Retrospect is Not Open: To change the magazine when Retrospect is not open you need not take any special action.

  Tape Slot Numbers: The magazine has five slots, numbered 0 through 4; ignore these numbers. Consider the magazine slots numbered 1 through 5, corresponding to Retrospect's slot numbers.

Quantum DLT2700 through -4700 series:
  A seven-tape Quantum DLT library has four modes which are set using the key on the front of the loader. The modes are Locked, Automatic, Manual, and Service, with each mode's key position designated by an icon. To work with Retrospect, the library must be in Locked or Automatic mode.

  Changing the Magazine when Retrospect is Open: To eject the magazine, first choose Eject Magazine from Retrospect's devices toolbar. Turn the loader's key to the Automatic position and, after the green light on the loader's Eject button illuminates, press the button. When the door opens, tilt it down to its fully open position and remove the magazine. Load the magazine completely with your desired tapes, replace the magazine in the loader, turn the key to the Locked position, then push the door closed. The first tape is automatically loaded into the drive.

  Changing the Magazine when Retrospect is Not Open: To change the magazine when Retrospect is not open you need not take any special action.

  Tape Slot Numbers: The library's door has a number for each tape slot, numbered 0 through 6; ignore these numbers. Consider the magazine slots numbered 1 through 7, corresponding to Retrospect's slot numbers.

Seagate Sidewinder 200:
  To clean this loader's drive, first insert a cleaning cartridge in the magazine and insert the magazine in the loader. Then, using the buttons on the front panel, select the slot containing the cleaning tape. When the cleaning cartridge is loaded in the drive, it automatically cleans the drive. Eject the magazine and replace the cleaning cartridge with a tape cartridge.

Sony TSL-A300c, Cybernetics CY-TL8-1004:
  To clean this loader's drive, first insert a cleaning cartridge in the magazine and insert the magazine in the loader. Then, using the buttons on the front panel, select the slot containing the cleaning tape. When the cleaning cartridge is loaded in the drive, it automatically cleans the drive. Eject the magazine and replace the cleaning cartridge with a tape cartridge.

Copyright © 2000 Dantz Development Corporation