Specification

x Chat has been tested with the following environment.

OS Memory Processor Modem Network Card Monitor Sound Card | : Windows 95/98/NT4 with TCP/IP protocol setup properly: : 64 MB * : Pentium 133 (Celeron, Pentium II or faster processor is recommended)** : Cable modem (Optional)*** : 10Base2, 100 Base-T, 100Base-Tx (Support up to 5 NICs) : Support 16 bit colour (65535 colours) :: Required for Attention Bell

* x Chat requires about 6 Mb maximum windows memory
** it will have better performance with a Pentium II level processor and high speed connection.
***For advanced user to use x Chat in the Internet.