
                          Additional Information

                        Multimedia Pro 16ABO V1.10


   This file contains additional information and changes about the
   various software that was not available at printing time.

   Win95 driver Installation for Sound Card
   =========================================

   1. Start the Windows 95 program.  Click on the <Start> button on the bottom 
   taskbar, select <Setting> from the menu and click on the <Control Panel>
   selection.

   2. Select <Add New Hardware> under Control Panel menu.  Click on the <Next> 
   button and select <No> from "Add New Hardware" the screen and click on 
   the <Next> button again.  Adjust the scroll bar to "Sound,video and game 
   Controllers" menu line and select it. 

   3. Click on the <Next> button, followed by the <Have Disk> button. You will 
   be prompted to insert Driver disk into A:\.  

   4. You should insert the sound card Audio Disk #1 into the Drive A: (B:)
   and path it to \WIN95 directory drive to continue the installation of 
   the Windows 95 16-bit audio drivers. This will end the sound card drivers
   installation.

   5. To make use of the WaveTable/External MIDI devices and joystick port. You 
   should proceed to install the drivers for MPU-401 and joystick. To install 
   these drivers, repeat steps #1 to #2 and shift the scroll bar downward to 
   select "Microsoft" from the Manufactuers box. A list of drivers will now 
   be displayed in the "Models:" dialog box.  Click on MPU401 & joystick one 
   at a time to complete the installation.
   (Note: MPU-401 & joystick drivers can be found in your Win95 CD-ROM.)

   6. Restart the Win95 session to effect the newly installed drivers.

   7. If you encounter any conflict after installation, please refer to the 
   Trouble-shooting section in Win95 for further details.


   Aztech IDE CD-ROM Drive Installation
   ====================================

   If you are connecting the CD-ROM drive to your primary IDE interface,
   include the following statement in the Windows file SYSTEM.INI under
   the [Enh386] section:

        32BitDiskAccess=Off


   Microsoft CD-ROM Extensions (MSCDEX.EXE)
   ========================================

   The above file is needed for operation of CD-ROM drives under the DOS
   environment. This file is only bundled with DOS version 6.x. Therefore, 
   if you are using DOS version 5, please contact your local Microsoft's
   dealers for a copy of MSCDEX.EXE (for DOS version 5 usage).


   
   Using Digital (.WAV) Audio with DOS 6.x's DoubleSpace*
   ======================================================

   The DoubleSpace utility included with DOS 6.x can cause problems
   if you attempt to play or record "high data rate" (i.e.: stereo/
   44.1kHz/16-bit) digital audio to or from a compressed disk.

   Therefore, if you anticipate that you will be playing or recording
   a lot of stereo/44.1kHz/16-bit digital audio, you should set up a
   non-compressed drive partition and configure the audio application
   to use this drive as their Work and Temp directories. 

   For information on setting up a non-compressed partition for your
   hard drive, refer to your DOS 6.x Users Guide. 

   *The same procedure should be followed if you are using Stacker, a
   third-party disk compression utility.


   Notes About Using EMM386.EXE
   ============================

   When running applications with EMM386.EXE installed, the following
   error message may appear:

      "EMM386 DMA buffer is too small"

   You can overcome this problem in two ways:

      - remove the EMM386.EXE entry from the CONFIG.SYS file

      OR

      - add the following parameter to the EMM386.EXE entry in the
        CONFIG.SYS file:

           D=64

           where D specifies how many kilobytes of memory should be
           reserved for buffered Direct Memory Access (DMA).

        An example of this may be:

           C:\WINDOWS\EMM386.EXE D=64

         
     *************************************************************
     *    In case you encounter any problem with our products,   *
     *    please quote the following model(s) when calling our   *
     *    Technical Support:                                     *
     *                        WASHINGTON 16ABO Sound Card        *
     *************************************************************

                            --- End of File ---

