The DUALMON utility is intended for those who have installed both
a primary VGA monitor and a secondary hercules mono monitor.

This driver has been released into the Public Domain. It is basing on
two drivers called COLR-DRV.SYS and MONO-DRV.SYS. Unfortunately I don't
know the original author. In the relating documentation I only found the
address of someone called Alan Barclay, but I could not contact him.
I presume, he moved from there.

  Alan Barclay
  iT                                |        E-mail : alan@ukpoit.uucp
  Barker Lane                       |        BANG-STYLE : .....!ukc!ukpoit!alan
  CHESTERFIELD S40 1DY              |        VOICE : +44 246 214265
  Derbys, England                   |        FAX   : +44 246 214353


The two drivers (in one .SYS file) allow output redirection to the
"other" monitor.
Example to use:
    If the VGA is the "current" monitor, you can display the output of DIR
    on the mono. monitor as follows:
        DIR>MONO

    Similarly if the mono. monitor is "current"
        DIR>COLOR
    will redirect output of DIR to the VGA.

Note that MODE can switch between the two monitors.
Ex:
    MODE MONO and MODE CO80

Install DUALMON.SYS via device= lines in CONFIG.SYS.
For example:
        device=c:\dualmon.sys

  Axel C. Frinke        ACFrinke@uni-bonn.de
  Steinstr.11           Axel-C_Frinke@su.maus.de (mails < 64KB only!)
D-53332 Bornheim

