

                    -+- Enlight the Surreal by Noice -+-

               - Released at Assembly2k in Helsinki Finland -
               - Placed 9:th in the demo compo
	       - non-accelerated, have fun!



-------------------------------------------------------------------------------
Legal Notice:
----------------------
This demo is free to spread and copy as much as you want. 
However, if you put this on a CD availible to the public in any way,
you must send us a copy. Program is provided as is, without any kind
of warranty.

-------------------------------------------------------------------------------
System requirements:
----------------------
* Pentium II 300 (or better), 64 Mb of RAM.
* Windows DirectX 3 or 7 (fullscreen/window) or failover through GDI.

-------------------------------------------------------------------------------
Main Credits:
----------------------
Demo Coding........: Gnilk, Krikkit
Graphics & Textures: Flood
Modelling..........: Rico
Font...............: Gaijin
Music..............: Evade, Martyn
Design.............: Gnilk, Flood
Additional stuff...: Gaijin


This demo uses:
----------------------
* BASS soundsystem by Ian Luck
* JPEG library Independent JPEG  Group
* truetype font library FreeType 
* ZLIB 1.1.3, (C) 1995-1998 Jean-loup Gailly and Mark Adler

-------------------------------------------------------------------------------
Some words from the authors:
--------------------------------
If you would like to contact us, go right ahead:

 * Gnilk   : gnilk@home.se
 * Krikkit : robertlu@csd.uu.se

-------------------------------------------------------------------------------
Greetings:
----------------------

  cryonics - fairlight - replay - obscure - outbreak - tmb - trauma
   doomsday - komplex - tbl - tazadum - amc - array - mass - yodel
-------------------------------------------------------------------------------
   For futher information and more detailed credits visit our web-site.


                www.noice.org - the center of goatology


// noiceteam -- 20000804
