3Com Corporation
3Com Megahertz 10/100 LAN CardBus PC Card 
NetWare DOS/ODI Driver Installation Information

WINDOWS 3.1X AND NOVELL NETWARE
This file describes how to configure the 3Com Megahertz 
10/100 LAN CardBus PC Card for use with 
Windows V3.1x (Not Windows for Workgroups) and Novell NetWare. 

NOTE: 
The following instructions assume you have not installed
any other network adapter in the notebook. If networking
has already been installed, some of the instructions will
not apply or appear accurate. Consult with your MIS 
department for further instructions.

Before installing the network driver, you should know the 
transport used in the Novell Network (typically IPX/SPX) and
have access to the following software components:

    - Novell NetWare VLM Client disks for DOS and Windows
    - The LAn Installation Disk


Network Driver Installation Instructions

1.  Boot the notebook in DOS. If the PC starts up in Windows,
    exit Windows to return to the DOS prompt. 

2.  Place the Novell VLM client disk #1 in the floppy drive. Enter:

        a:\install

    This opens the NetWare client installation screen.
    Use the down arrow key to move from line-to-line. 

3.  Make sure that the information is correct. 
    When you are asked to select the driver for 
    your network card, press <Enter> to see the
    list of supported adapters. 
    
4.  Select Other Drivers.

4.  When prompted for a driver disk, 
    insert the LAN Installation Disk and press <Enter>. 

    FE575C-3Com 10/100 LAN CardBus -Fast Ethernet 
    should appear as the first item on the
    list. 

5.  Select the CardBus PC Card and press <ENTER>.

6.  Specify the frame type by pressing <ENTER> and choosing the
    appropriate type from the list. Press <Enter> to select your
    choice. (You will not need to select an I/O Base. Use the
    default.)

7.  Press F10 to return to the main installation screen. Position
    the cursor on line 6 and press <Enter>. The installer
    prompts for several diskettes and notifies you when the
    installation is complete.

8.  Press <Enter> to exit the installation program and return to DOS.

9.  Reboot the notebook by pressing <CTRL><ALT><DEL>. When you 
    go into Windows You will be able to LOGIN to the 
    Novell Servers.

%VER Version 2.6.1.01