3Com Corporation
3Com Megahertz 10/100 LAN CardBus PC Card
Windows for Workgroups Novell Driver Installation Information

WINDOWS FOR WORKGROUPS v3.11 AND NOVELL NETWARE

This file describes how to configure the PC Card for
use with Windows for Workgroups v3.11 and Novell NetWare.

NOTE: The following instructions assume that you have not
      installed any other network adapter in the notebook. If you
      have been using a network connection on your notebook,
      some of the following instructions may not apply or may
      produce different results. Refer to your MIS department
      or system manager for further instructions.

Before installing the network driver, you should know:

      - The Frame type used in the network 
       (802.2 is the default).
      - The name of your Novell file server.
      - Obtain the Novell NetWare VLM Client disks 
        for DOS and Windows 
      - PC Card and the LAN Installation Disk
     
Installation Instructions:

1.  Boot the system in DOS. If the system starts up in windows,
    close Windows and exit to DOS.

2.  Place the Novell VLM Client disk #1 in the floppy drive and
    enter:

        a:install

3.  This opens the NetWare Client Installation window. Use the
    arrow keys to move between fields. Verify that the
    information on each line is correct.

4.  In the field asking you to select the driver for your network
    card, press Enter to see the list of support drivers. At the
    bottom of the list, select OTHER DRIVERS and press Enter.

5.  At the prompt for a driver disk, put the EtherDisk in your
    floppy drive, and press Enter 3Com Megahertz LAN CardBus 
    PC Card and press Enter.

6.  Select the frame type by pressing Enter and choosing the
    appropriate type from the list. After your selection is made,
    press Enter again. You will not need to select an "I/O
    Base", as the default is appropriate for our drivers. Press
    F10 to return to the main installation screen.

7.  To install the driver, select line 6 from this screen and
    press Enter. During the installation process, you 
    will be asked for specific floppy diskettes. Follow the
    instructions on the screen. When the installer finishes,
    press Enter.

8. Reboot the notebook.

%VER Version 2.6.1.01