3Com Corporation
3Com Megahertz 10/100 LAN CardBus PC Card 
IBM LAN Server 4.0 for DOS Installation Information


IBM DOS LAN Services Install v4.0

1.  Insert the disk labeled "DOS LAN Services Disk 1" into 
     your floppy disk drive.

2.  Enter: 
    A:INSTALL

3.  Choose the directory where you want the software installed.
    The default is C:\NET.

4.  A menu provides a list of  Network Cards.
    Choose "Network card not shown in the list below..." 

5.  Remove the  DOS LAN Services Disk 1 diskette,  insert 
    the LAN Installation Disk, and enter: 
    A:\NDIS2

    The next menu shows 3Com Megahertz 10/100 LAN 
    CardBus PC Card.

6.  Additional menus appear. 
    Choose the appropriate options for your network 
    environment. 

    Refer to your IBM manual if you have questions 
    regarding these menus.

7.  After completing the installation you must copy ELPC575.DOS 
    to C:\NET before rebooting.

%VER Version 2.6.1.01