3Com Corporation
3Com Megahertz 10/100 LAN CardBus PC Card
Banyan Vines Information


Banyan VINES
------------

To install VINES 6.0 software on a DOS NDIS 
workstation, follow these instructions.  

DOS must be installed on the target workstation 
C: drive, or you must have a bootable DOS floppy. 

Before you begin, you must have the IRQ for the PC Card.
To display the configuration, see the INSTRUCT.TXT file.

1.  Use the DOS MD command to create a subdirectory 
    called \VINES.

2.  Copy the contents of the VINES LAN S/W (DOS) 
    LAN Installation Disk into the \VINES subdirectory.

3.  Copy the contents of the NDIS subdirectory on 
    the VINES LAN S/W (DOS) 2 of 2 diskette into 
    the \VINES subdirectory.

4.  Copy the ELPC575.DOS from 
    A:\MSLANMAN.DOS\DRIVERS\ETHERNET\ELPC575
    directory on the 
    LAN Installation Disk to the C:\VINES subdirectory.

5.  Copy the PROTOCOL.INI fragment from the 
    \MSLANMAN.DOS\DRIVERS\ETHERNET\ELPC575 subdirectory
    on the LAN Installation Disk to the \VINES subdirectory.

6.  Edit the PROTOCOL.INI file to read as follows:

     [PROTOCOL MANAGER]
      DRIVERNAME = PROTMAN$

     [VINES_XIF]
      DRIVERNAME = NDISBAN$
      BINDINGS = ELPC575

     [ELPC575]
      DRIVERNAME = ELPC575$
         
7.  Run the PCCONFIG.EXE program located in the 
    \VINES subdirectory.

8.  Select option 1, Network Card Settings.

9.  Select the NDIS Ethernet option.

10. The NDIS workstation screen appears.  Enter 
    the IRQ that you selected for the PC Card. 
    Select the IRQ using the Configuration
    and Diagnostic Program. 

11. Press F10 twice to return to the first menu.

12. On the next screen, select option 2, Login 
    Environment Settings.

13. On the next screen, select option 1, Default 
    Communications Driver.

14. On the next screen scroll down to NDIS Ethernet 
    and press Enter.

15. Exit PCCONFIG by pressing [F10] to save the new 
    configuration.

16. Edit the CONFIG.SYS file and add the following 
    lines, substituting A: for C: for a floppy 
    disk installation.
                                   
     DEVICE = C:\VINES\PROTMAN.DOS /I:C:\VINES
     DEVICE = C:\VINES\ELPC575.DOS
     LASTDRIVE = M

17. Edit the AUTOEXEC.BAT file and add the following
    lines:

     CD\VINES
     BAN
     CD\

     BAN loads the NDISBAN drivers and reads the 
     PCCONFIG.OBJ file to activate changes made during the
     PCCONFIG stage.

%VER Version 2.6.1.01