PCE-ATARIST(1)                        pce                       PCE-ATARIST(1)



NAME
       pce-atarist - Atari ST emulator

SYNOPSIS
       pce-atarist [options]

DESCRIPTION
       pce-atarist(1) is an Atari ST emulator.

OPTIONS
       -c, --config file
              Set the config file name.

       -d, --path string
              Add a directory to the search path.

              The search path is used if an input file (such as a ROM image or
              a disk image) is specified with a relative file  name.  In  that
              case  the  file is searched for in all directories of the search
              path. The current directory is always implicitly  added  to  the
              end of the search path.

              The directory name can be prefixed by one of these characters:

              +      Add the directory to the end of the search path

              -      Add the directory to the beginning of the search path

              =      Clear the search path before adding the directory


              The  default  is  to  add the directory to the end of the search
              path.

       -i, --ini-prefix string
              Parse string as if it were added to the beginning of the  config
              file.

       -I, --ini-append string
              Parse string as if it were added to the end of the config file.

       -l, --log file
              Write log messages to the file specified instead of stdout.

       -p, --cpu model
              Select the CPU model to be emulated, overriding the config file.
              Possible values for model are 68000, 68010 and 68020.

       -q, --quiet
              Don't print anything to stdout or stderr.

       -r, --run
              Start running immediately.

       -R, --no-monitor
              Start running immediately and never fall back  to  the  monitor.
              This is useful if stdout is not visible, for example because the
              emulator was started directly from a  graphical  user  interface
              such as X or Windows.

       -s, --speedfactor
              Set  the  initial speed factor. This overrides a value specified
              in the configuration file.

       -t, --terminal string
              Set the terminal device. Possible devices are null, x11 and sdl.

       -v, --verbose
              Verbose operation. This is highly recommended.

       --help Print usage information

       --version
              Print version information

SEE ALSO
       pri(1), psi(1)

AUTHOR
       Hampa Hug <hampa@hampa.ch>



HH                                2013-08-19                    PCE-ATARIST(1)
