                            INSTALLATION OVERVIEW

This file lists the steps necessary to install the Above Board 286 and PS/286.
For details about each of these steps, refer to the Above Board manual.

1  Add memory to the Above Board.  The board can hold as much as 2M bytes.

2  Insert the Above Board in the computer.

3  Run the SETBOARD program to set up the board's hardware.

4  Run the computer's setup program (for 80286-based computers only) if you
   use the Above Board to add conventional or extended memory.

5  Run the TESTAB (confidence tests) program to pinpoint non-functioning or
   improperly installed RAM chips on the Above Board.

6  Run the INSTALL program to install the Above Board software that lets you
   use expanded memory, RAM disks, and a print buffer.  

7  Run the CHKMEM program to list the amount of conventional, expanded,
   and extended memory in your computer.

