   Windows 95 Installation
Installation
1.   Boot up Windows 95
2.   In windows 95 "Booted" Screen., select "Start" item.
     select "Start" item.
3.   In "Start" Screen,
     select "Settings" item.
4.   In "Settings" Screen,
     select "Control Panel" item.
5.   In "Control Panel" Screen,
     select "Display" icon.
6.   In "Display Properties" Screen,
     select "Settings" item.
7.   In "Display Properties" Screen,
     select "Change Display Type" item.
8.   In "Change Display Type" Screen,
     select "Adapter type => Change" item.
9.   In "Select Device" Screen,
     select "Have Disk...." item.
10.  In "Install From Disk" Screen,
     select your driver source.
     e.g.  A:\WIN95
11.  In new "Select Device" Screen,
     "S3 ViRGE" would appear and
     select "OK"
     Then Windows 95 would perform driver installation.
12.  After completing installation,
     Windows 95 would go back to "Change Display Type" Screen,
     select "Close" item.
13.  Windows 95 would go back to "Display Properties" Screen and you may select
     desired resolution by changing "Desktop area" pointer,
     desired color by changing "Color Palette" value, and
     desired font size by changing "Font size"
14.  After completing selection,
     choose "Apply" to complete the whole installation.
15.  Then Windows 95 would ask
     "Do you want to restart Windows ?"
     Choose "Restart" to make your selection active and you may work at your
     selection mode.

