REM file: QBX.BI for Hex Editor v4.8a
REM BIOS Interrupt structure

Type RegTypeX
 AX As Integer ' A register
 BX As Integer ' B register
 CX As Integer ' C register
 DX As Integer ' D register
 BP As Integer ' base pointer
 SI As Integer ' source index
 DI As Integer ' destination index
 Flags As Integer ' cpu flags
 DS AS Integer ' data segment
 ES AS Integer ' extra segment
End Type

Declare Sub InterruptX(N AS Integer,I AS RegTypeX,O AS RegTypeX)
