3Com Corporation
3Com Megahertz 10/100 LAN CardBus PC Card (3CCFE575CT)

3Com's Intelligent Auto Install software, ComsLink,
copies the NetWare DOS Requester software from the LAN
Installation Disk to the system you are configuring
for NetWare.  You may have newer versions of this
software from another source.  If so, the Comslink
program can download the NetWare client software from
the server instead of the LAN Installation Disk. This
feature can be used to install newer versions of the
software or to customize your installation.

Comslink can also install basic Netware support for
Windows 3.1X and Windows For Workgroups 3.11.  These
two options can be specified by using install.exe in
the root directory of the LAN Installation Disk.

ComsLink installs the NetWare client software from the
LAN Installation Disk, then starts it, and connects to
a server.  Once connected, ComsLink looks in the LOGIN
directory of the server for a file called
3INSTALL.BAT.  If this file exists, ComsLink will
spawn it.

If you want to deliver installations specific to your
environment, your system administrator can create a
batch file named 3INSTALL.BAT to copy specific
software required during your client installation
process.  For example, you may have multiple
protocols, unique configurations, special application
software, or non-NetWare clients in your network
environment.

When using ComsLink, be sure your diskette is not
write-protected.

For instructions on how to use ComsLink, see the user guide.

%ver 2.6.1.02