;****************************************************************************************
;
; RT61.inf
;
;   This installation script supports Windows XP 64 Bit OS for the
;   Ralink RT2561 & RT2661 series Wireless LAN Card.
;
;   Copyright (C) @ 2002-2009 Ralink Technology Corporation. All Rights Reserved.
;   All Rights Reserved.
;   Developed by RaLink Technology, Corp. -- http://www.ralinktech.com
;
;****************************************************************************************

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %Ralink%
Compatible      = 1
DriverVer       = 06/12/2009, 1.02.08.0000
CatalogFile     = RT61.CAT            

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%Ralink%        = Ralink, NTamd64
%Gigabyte%      = Gigabyte, NTamd64
%Edimax%        = Edimax, NTamd64
%Sitecom%       = Sitecom, NTamd64
%Delta%         = Delta, NTamd64
%Hawking%       = Hawking, NTamd64
%Billionton%    = Billionton, NTamd64
%Asus%          = ASUS, NTamd64
%ZINWELL%       = ZINWELL, NTamd64
%AMIT%          = AMIT, NTamd64
%CASTLENET%     = CASTLENET, NTamd64
%ACCTON%        = ACCTON, NTamd64
%Surecom%       = Surecom, NTamd64
%Belkin%        = Belkin, NTamd64
%VTech%         = VTech, NTamd64
%Siemens%       = Siemens, NTamd64
%Conceptronic%  = Conceptronic, NTamd64
%SMC%           = SMC, NTamd64
%CNet%          = CNet, NTamd64
%Corega%        = Corega, NTamd64
%Netopia%       = Netopia, NTamd64
%AboCom%        = AboCom, NTamd64
%Planex%        = Planex, NTamd64
%Logitec%       = Logitec, NTamd64
%Corega2%       = Corega2, NTamd64

[Ralink.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Ralink_0301.DeviceDesc%    = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_25611814
%Ralink_0302.DeviceDesc%    = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_25611814
%Ralink_0401.DeviceDesc%    = RALINK_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_26611814
; MSI
%M61_B833T.DeviceDesc%      = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_B8331462
%M61_B834T.DeviceDesc%      = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_B8341462
%M61_B835T.DeviceDesc%      = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_B8351462
%M61_B833.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_B8331462
%M61_B834.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_B8341462
%M61_B835.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_B8351462
%M61_C855.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_C8551462
; Winstron
%WLANm.DeviceDesc%          = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_12A0185F
%WLANc.DeviceDesc%          = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_22A0185F
; Amigo
%AMIGO_9142.DeviceDesc%     = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_914216EF
%AMIGO_9222.DeviceDesc%     = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_922216EF
%AMIGO_9262.DeviceDesc%     = RALINK_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_926216EF
%AMIGO_9142V2.DeviceDesc%   = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_914216EF
%AMIGO_9221.DeviceDesc%     = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_922116EF
%AMIGO_9261.DeviceDesc%     = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_926116EF
%AMIGO_9223.DeviceDesc%     = RALINK_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_922316EF
; CNet
%CNetPCI.DeviceDesc%        = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_00251371
%CNetMPCI.DeviceDesc%       = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_00261371
%CNetCardbus.DeviceDesc%    = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_00271371
; Qcom
%Qcom.DeviceDesc%           = RALINK_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_619418E8

[Gigabyte.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%GigabyteWM01GS.DeviceDesc% = GIGABYTE1.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_E8321458
%GigabyteWI01GS.DeviceDesc% = GIGABYTE1.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_E9331458
%GigabyteWP01GS.DeviceDesc% = GIGABYTE1.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_E9341458
%GigabyteWM02GS.DeviceDesc% = GIGABYTE2.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_E8321458
%GigabyteWI02GS.DeviceDesc% = GIGABYTE2.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_E9331458
%GigabyteWP02GS.DeviceDesc% = GIGABYTE2.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_E9341458
%GigabyteWI02GM.DeviceDesc% = GIGABYTE3.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_E9351458
%GigabyteWM01GM.DeviceDesc% = GIGABYTE3.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_E8331458
%GigabyteWP01GM.DeviceDesc% = GIGABYTE3.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_E9361458

[Edimax.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%EW-0301-7108.DeviceDesc%   = Edimax_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_71081432
%EW-0301-7128.DeviceDesc%   = Edimax_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_71281432
%EW-7108.DeviceDesc%        = Edimax_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_71081432
%EW-7128.DeviceDesc%        = Edimax_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_71281432
%EW-7608.DeviceDesc%        = Edimax_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_76081432
%EW-7628.DeviceDesc%        = Edimax_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_76281432

[Sitecom.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Sitecom_WL112V2.DeviceDesc% = SITECOM_0301.ndi,         PCI\VEN_1814&DEV_0301&SUBSYS_9072182D
%Sitecom_WL115V2.DeviceDesc% = SITECOM_0301.ndi,         PCI\VEN_1814&DEV_0301&SUBSYS_9074182D
%Sitecom_WL170.DeviceDesc%  = SITECOM_0301.ndi,     PCI\VEN_1814&DEV_0301&SUBSYS_90AA182D
%Sitecom_WL171.DeviceDesc%  = SITECOM_0301.ndi,     PCI\VEN_1814&DEV_0301&SUBSYS_90AB182D
%Sitecom_WL211.DeviceDesc%  = SITECOM_0301.ndi,     PCI\VEN_1814&DEV_0301&SUBSYS_0025182D
%Sitecom_WL210.DeviceDesc%  = SITECOM_0301.ndi,     PCI\VEN_1814&DEV_0301&SUBSYS_0026182D
%Sitecom_WL150.DeviceDesc%  = SITECOM_0401.ndi,          PCI\VEN_1814&DEV_0401&SUBSYS_9096182D
%Sitecom_WL151.DeviceDesc%  = SITECOM_0401.ndi,          PCI\VEN_1814&DEV_0401&SUBSYS_9097182D

[Delta.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DeltaPCI.DeviceDesc%       = DELTA.ndi,            PCI\VEN_1814&DEV_0301&SUBSYS_701C4033
%DeltaCB.DeviceDesc%        = DELTA.ndi,            PCI\VEN_1814&DEV_0301&SUBSYS_701B4033

[Hawking.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Hawking0C54.DeviceDesc%    = HAWKING.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_0C541432
%Hawking0B54.DeviceDesc%    = HAWKING.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_0B541432

[Billionton.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%GMIWLGRL2-B.DeviceDesc%   = BILLIONTON.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_020514CB
%GMIWLGRL2-N.DeviceDesc%   = BILLIONTON.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_020614CB

[ASUS.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ASUS_837E.DeviceDesc%      = ASUS_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_837E1043
%ASUS.DeviceDesc%           = ASUS_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_107F1043
%ASUS.DeviceDesc%           = ASUS_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_127F1043
%ASUS.DeviceDesc%           = ASUS_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_130F1043
%ASUS.DeviceDesc%           = ASUS_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_137F1043
%ASUSGEN.DeviceDesc%        = ASUS_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_137E1043

[ZINWELL.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ZINWELLPCI.DeviceDesc%     = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_03615A57
%ZINWELLMPCI.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_03605A57
%ZINWELLCARD.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_01605A57
%ZINWELLOEM1.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_300918A3
%ZINWELLOEM2.DeviceDesc%    = ZINWELL.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_301018A3

[AMIT.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AMIT.DeviceDesc%           = AMIT_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_531018EB
%AMITMINI.DeviceDesc%       = AMIT_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_531118EB
%AMITPCI.DeviceDesc%        = AMIT_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_531218EB
%AMIT0100.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_010018EB
%AMIT0200.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020018EB
%AMIT0300.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030018EB
%AMIT0202.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020218EB
%AMIT0302.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030218EB
%AMIT0203.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020318EB
%AMIT0303.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030318EB
%AMIT0204.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_020418EB
%AMIT0304.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_030418EB
%AMITCG.DeviceDesc%         = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_C11E1259
%AMIT0006.DeviceDesc%       = AMIT_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_000618C5

[CASTLENET.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CASTLENET.DeviceDesc%      = CASTLENET.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_12801688

[ACCTON.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%WN4306A.DeviceDesc%        = WN4306A.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_43061113

[Surecom.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SurecomPCI.DeviceDesc%     = SURECOM.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_13F310BD
%SurecomCardbus.DeviceDesc% = SURECOM.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_14F310BD

[Belkin.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Belkin.DeviceDesc%         = BELKIN_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_701A1799
%Belkin.DeviceDesc%         = BELKIN_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_700A1799
%Belkin_901B.DeviceDesc%    = BELKIN_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_901B1799
%Belkin_901C.DeviceDesc%    = BELKIN_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_901C1799
%Belkin_700E.DeviceDesc%    = BELKIN_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_700E1799
%Belkin_700E.DeviceDesc%    = BELKIN_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_700E1799
%Belkin_701E.DeviceDesc%    = BELKIN_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_701E1799
%Belkin_701E.DeviceDesc%    = BELKIN_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_701E1799

[VTech.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%VTechPCI.DeviceDesc%       = VTECH.ndi,            PCI\VEN_1814&DEV_0302&SUBSYS_301118A3
%VTechCARD.DeviceDesc%      = VTECH.ndi,            PCI\VEN_1814&DEV_0302&SUBSYS_301318A3

[Siemens.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Siemens.DeviceDesc%        = SIEMENS.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_3C800681

[Conceptronic.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Conceptronic_PCCard.DeviceDesc% = CONCEPTRONIC.ndi,  PCI\VEN_1814&DEV_0302&SUBSYS_3C231948
%Conceptronic_PCICard.DeviceDesc% = CONCEPTRONIC.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_3C241948

[SMC.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SMC_EE04.DeviceDesc%       = SMC.ndi,              PCI\VEN_1814&DEV_0401&SUBSYS_EE041113
%SMC_EE05.DeviceDesc%       = SMC.ndi,              PCI\VEN_1814&DEV_0401&SUBSYS_EE051113

[CNet.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%CNet_6221.DeviceDesc%      = CNET_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_62211371
%CNet_7221.DeviceDesc%      = CNET_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_72211371
%CNet_8221.DeviceDesc%      = CNET_0301.ndi,        PCI\VEN_1814&DEV_0301&SUBSYS_82211371
%CNet_6121.DeviceDesc%      = CNET_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_61211371
%CNet_7121.DeviceDesc%      = CNET_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_71211371
%CNet_8121.DeviceDesc%      = CNET_0302.ndi,        PCI\VEN_1814&DEV_0302&SUBSYS_81211371
%CNet_6321.DeviceDesc%      = CNET_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_63211371
%CNet_7321.DeviceDesc%      = CNET_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_73211371
%CNet_8321.DeviceDesc%      = CNET_0401.ndi,        PCI\VEN_1814&DEV_0401&SUBSYS_83211371

[Corega.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega.DeviceDesc%         = Corega.ndi,           PCI\VEN_1814&DEV_0401&SUBSYS_C11D1259

[Netopia.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Netopia.DeviceDesc%        = Netopia.ndi,          PCI\VEN_1814&DEV_0302&SUBSYS_914116EF

[AboCom.NTamd64]
; DisplayName                    Section                 DeviceID
; -----------                    -------                 --------
%AboCom_0301_ABA1.DeviceDesc%    = AboCom_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_ABA113D1
%AboCom_0301_ABA2.DeviceDesc%    = AboCom_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_ABA213D1
%AboCom_0301_ABA4.DeviceDesc%    = AboCom_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_ABA413D1
%AboCom_0301_ABA5.DeviceDesc%    = AboCom_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_ABA513D1
%AboCom_0301_ABE3.DeviceDesc%    = AboCom_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_ABE313D1
%AboCom_0301_ABE4.DeviceDesc%    = AboCom_0301.ndi,      PCI\VEN_1814&DEV_0301&SUBSYS_ABE413D1
%AboCom_0302_ABA1.DeviceDesc%    = AboCom_0302.ndi,      PCI\VEN_1814&DEV_0302&SUBSYS_ABA113D1
%AboCom_0401_ABA7.DeviceDesc%    = AboCom_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_ABA713D1
%AboCom_0401_ABA1.DeviceDesc%    = AboCom_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_ABA113D1
%AboCom_0401_ABA3.DeviceDesc%    = AboCom_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_ABA313D1
%AboCom_0401_ABE5.DeviceDesc%    = AboCom_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_ABE513D1
%AboCom_0401_ABA6.DeviceDesc%    = AboCom_0401.ndi,      PCI\VEN_1814&DEV_0401&SUBSYS_ABA613D1

[Planex.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Planex.DeviceDesc%         = Planex.ndi,           PCI\VEN_1814&DEV_0401&SUBSYS_AB1914EA

[Logitec.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Logitec.DeviceDesc%        = Logitec.ndi,          PCI\VEN_1814&DEV_0301&SUBSYS_002C6409

[Corega2.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%Corega2.DeviceDesc%        = Corega2.ndi,          PCI\VEN_1814&DEV_0301&SUBSYS_C1231259

;*******************************************************************************************
; NT specific entries
;*******************************************************************************************

[RALINK_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[RALINK_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE1.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE2.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[GIGABYTE3.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Edimax_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SITECOM_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SITECOM_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[DELTA.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[HAWKING.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[BILLIONTON.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ASUS_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ASUS_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[ZINWELL.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIT_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AMIT_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CASTLENET.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[WN4306A.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SURECOM.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[BELKIN_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[BELKIN_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[BELKIN_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[VTECH.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SIEMENS.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CONCEPTRONIC.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[SMC.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[CNET_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Corega.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Netopia.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AboCom_0301.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AboCom_0302.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[AboCom_0401.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Planex.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Logitec.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

[Corega2.ndi.NT]
AddReg                  = Common.reg, RT61.ndi.NT.reg, Customer1.reg
Characteristics         = 0x84                      ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5
CopyFiles               = NT.CopyFiles

; NT services sections
[RALINK_0301.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[RALINK_0302.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[RALINK_0401.ndi.NT.Services]
AddService              = RT61, 2, RALINK.Service, common.EventLog

[GIGABYTE1.ndi.NT.Services]
AddService              = RT61, 2, GIGABYTE.Service, common.EventLog

[GIGABYTE2.ndi.NT.Services]
AddService              = RT61, 2, GIGABYTE.Service, common.EventLog

[GIGABYTE3.ndi.NT.Services]
AddService              = RT61, 2, GIGABYTE.Service, common.EventLog

[Edimax_0301.ndi.NT.Services]
AddService              = RT61, 2, Edimax.Service, common.EventLog

[Edimax_0302.ndi.NT.Services]
AddService              = RT61, 2, Edimax.Service, common.EventLog

[Edimax_0401.ndi.NT.Services]
AddService              = RT61, 2, Edimax.Service, common.EventLog

[SITECOM_0301.ndi.NT.Services]
AddService              = RT61, 2, SITECOM.Service, common.EventLog

[SITECOM_0401.ndi.NT.Services]
AddService              = RT61, 2, SITECOM.Service, common.EventLog

[DELTA.ndi.NT.Services]
AddService              = RT61, 2, DELTA.Service, common.EventLog

[HAWKING.ndi.NT.Services]
AddService              = RT61, 2, HAWKING.Service, common.EventLog

[BILLIONTON.ndi.NT.Services]
AddService              = RT61, 2, BILLIONTON.Service, common.EventLog

[ASUS_0301.ndi.NT.Services]
AddService              = RT61, 2, ASUS.Service, common.EventLog

[ASUS_0302.ndi.NT.Services]
AddService              = RT61, 2, ASUS.Service, common.EventLog

[ZINWELL.ndi.NT.Services]
AddService              = RT61, 2, ZINWELL.Service, common.EventLog

[AMIT_0302.ndi.NT.Services]
AddService              = RT61, 2, AMIT.Service, common.EventLog

[AMIT_0401.ndi.NT.Services]
AddService              = RT61, 2, AMIT.Service, common.EventLog

[CASTLENET.ndi.NT.Services]
AddService              = RT61, 2, CASTLENET.Service, common.EventLog

[WN4306A.ndi.NT.Services]
AddService              = RT61, 2, WN4306A.Service, common.EventLog

[SURECOM.ndi.NT.Services]
AddService              = RT61, 2, SURECOM.Service, common.EventLog

[BELKIN_0301.ndi.NT.Services]
AddService              = RT61, 2, BELKIN.Service, common.EventLog

[BELKIN_0302.ndi.NT.Services]
AddService              = RT61, 2, BELKIN.Service, common.EventLog

[BELKIN_0401.ndi.NT.Services]
AddService              = RT61, 2, BELKIN.Service, common.EventLog

[VTECH.ndi.NT.Services]
AddService              = RT61, 2, VTECH.Service, common.EventLog

[SIEMENS.ndi.NT.Services]
AddService              = RT61, 2, SIEMENS.Service, common.EventLog

[CONCEPTRONIC.ndi.NT.Services]
AddService              = RT61, 2, CONCEPTRONIC.Service, common.EventLog

[SMC.ndi.NT.Services]
AddService              = RT61, 2, SMC.Service, common.EventLog

[CNET_0301.ndi.NT.Services]
AddService              = RT61, 2, CNET.Service, common.EventLog

[CNET_0302.ndi.NT.Services]
AddService              = RT61, 2, CNET.Service, common.EventLog

[CNET_0401.ndi.NT.Services]
AddService              = RT61, 2, CNET.Service, common.EventLog

[Corega.ndi.NT.Services]
AddService              = RT61, 2, COREGA.Service, common.EventLog

[Netopia.ndi.NT.Services]
AddService              = RT61, 2, NETOPIA.Service, common.EventLog

[AboCom_0301.ndi.NT.Services]
AddService              = RT61, 2, General.Service, common.EventLog

[AboCom_0302.ndi.NT.Services]
AddService              = RT61, 2, General.Service, common.EventLog

[AboCom_0401.ndi.NT.Services]
AddService              = RT61, 2, General.Service, common.EventLog

[Planex.ndi.NT.Services]
AddService              = RT61, 2, General.Service, common.EventLog

[Logitec.ndi.NT.Services]
AddService              = RT61, 2, General.Service, common.EventLog

[Corega2.ndi.NT.Services]
AddService              = RT61, 2, General.Service, common.EventLog

;*******************************************************************************************
; common regs for NT
;*******************************************************************************************

[Common.reg]
;*******************************************************************************************
; System Level Property

;
; Current Profile
;
HKR, ,                    CurProfile,      0,""
HKR, Default,             CurProfile,      0,""

;
; Radio On/Off
;
HKR, ,                            Radio,           0, "0"
HKR, NDI\params\Radio,            ParamDesc,       0, %RadioOnOff%
HKR, NDI\params\Radio,            type,            0, "enum"
HKR, NDI\params\Radio,            default,         0, "0"
HKR, NDI\params\Radio\enum,       1,               0, %Disable%
HKR, NDI\params\Radio\enum,       0,               0, %Enable%

;
; Auto Reconnect Mode
;
HKR, ,                                  AutoReconnect,      0, "1"
HKR, NDI\params\AutoReconnect,          ParamDesc,          0, %AutoReconnectMode%
HKR, NDI\params\AutoReconnect,          type,               0, "enum"
HKR, NDI\params\AutoReconnect,          default,            0, "1"
HKR, NDI\params\AutoReconnect\enum,     0,                  0, %Disable%
HKR, NDI\params\AutoReconnect\enum,     1,                  0, %Enable%

;
; Show Hidden SSID in Site Survey Page
;
HKR, ,                                  ShowHiddenSSID,     0, "0"   ; 0=disable(default), 1=enable

;
; Country Region G Band
;
HKR, ,                                 CountryRegion,      0, "0"
HKR, NDI\params\CountryRegion,         ParamDesc,          0, %CountryRegion24G%
HKR, NDI\params\CountryRegion,         type,               0, "enum"
HKR, NDI\params\CountryRegion,         default,            0, "0"
HKR, NDI\params\CountryRegion\enum,    0,                  0, %CountryRegion24G_0%
HKR, NDI\params\CountryRegion\enum,    1,                  0, %CountryRegion24G_1%
HKR, NDI\params\CountryRegion\enum,    2,                  0, %CountryRegion24G_2%
HKR, NDI\params\CountryRegion\enum,    3,                  0, %CountryRegion24G_3%
HKR, NDI\params\CountryRegion\enum,    4,                  0, %CountryRegion24G_4%
HKR, NDI\params\CountryRegion\enum,    5,                  0, %CountryRegion24G_5%
HKR, NDI\params\CountryRegion\enum,    6,                  0, %CountryRegion24G_6%
HKR, NDI\params\CountryRegion\enum,    7,                  0, %CountryRegion24G_7%

;
; Country Region A Band
;
HKR, ,                                 CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand,    ParamDesc,          0, %CountryRegion5G%
HKR, NDI\params\CountryRegionABand,    type,               0, "enum"
HKR, NDI\params\CountryRegionABand,    default,            0, "0"
HKR, NDI\params\CountryRegionABand\enum,0,                 0, %CountryRegion5G_0%
HKR, NDI\params\CountryRegionABand\enum,1,                 0, %CountryRegion5G_1%
HKR, NDI\params\CountryRegionABand\enum,2,                 0, %CountryRegion5G_2%
HKR, NDI\params\CountryRegionABand\enum,3,                 0, %CountryRegion5G_3%
HKR, NDI\params\CountryRegionABand\enum,4,                 0, %CountryRegion5G_4%
HKR, NDI\params\CountryRegionABand\enum,5,                 0, %CountryRegion5G_5%
HKR, NDI\params\CountryRegionABand\enum,6,                 0, %CountryRegion5G_6%
HKR, NDI\params\CountryRegionABand\enum,7,                 0, %CountryRegion5G_7%
HKR, NDI\params\CountryRegionABand\enum,8,                 0, %CountryRegion5G_8%
HKR, NDI\params\CountryRegionABand\enum,9,                 0, %CountryRegion5G_9%
HKR, NDI\params\CountryRegionABand\enum,10,                0, %CountryRegion5G_10%

;*******************************************************************************************
; Advance Page

;
; OpMode
;
HKR, ,                            OpMode,          0, "0"

;
; WirelessMode
;
HKR, ,                            WirelessMode,    0, "3"

;
; Enable TX Burst
;
HKR, ,                            TXBurst,         0, "0"

;
; Use Short Slot Time
;
HKR, ,                            ShortSlot,       0, "1"

;
; Use Turbo rate
;
HKR, ,                            TurboRate,       0, "0"

;
; Use Ofdm rate in adhoc mode
;
HKR, ,                            AdhocOfdm,       0, "1"

;
; Use BG Protection
;
HKR, ,                            BGProtection,    0, "0"
HKR, NDI\params\BGProtection,           ParamDesc, 0, %BGProtection%
HKR, NDI\params\BGProtection,           type,      0, "enum"
HKR, NDI\params\BGProtection,           default,   0, "0"
HKR, NDI\params\BGProtection\enum,      0,         0, %Auto%
HKR, NDI\params\BGProtection\enum,      1,         0, %On%
HKR, NDI\params\BGProtection\enum,      2,         0, %Off%

;
; FrameAggregation
;
HKR, ,                            FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation,       ParamDesc, 0, %FrameAggregation%
HKR, NDI\params\FrameAggregation,       type,      0, "enum"
HKR, NDI\params\FrameAggregation,       default,   0, "1"
HKR, NDI\params\FrameAggregation\enum,  0,         0, %Disable%
HKR, NDI\params\FrameAggregation\enum,  1,         0, %Enable%

;
; IEEE80211H
;
HKR, ,                            IEEE80211H,      0, "0"
HKR, NDI\params\IEEE80211H,       ParamDesc,       0, %IEEE802_11h%
HKR, NDI\params\IEEE80211H,       type,            0, "enum"
HKR, NDI\params\IEEE80211H,       default,         0, "0"
HKR, NDI\params\IEEE80211H\enum,  0,               0, %Disable%
HKR, NDI\params\IEEE80211H\enum,  1,               0, %Enable%

;
; AutoChannelSelect
;
HKR, ,                            AutoChannelSelect,      0, "0"
HKR, NDI\params\AutoChannelSelect,       ParamDesc,0, %AutoChannelSelect%
HKR, NDI\params\AutoChannelSelect,       type,     0, "enum"
HKR, NDI\params\AutoChannelSelect,       default,  0, "0"
HKR, NDI\params\AutoChannelSelect\enum,  0,        0, %Disable%
HKR, NDI\params\AutoChannelSelect\enum,  1,        0, %Enable%

;
; WMMCapable
;
HKR, ,                            WMMCapable,      0, "0"
HKR, NDI\params\WMMCapable,             ParamDesc, 0, %WMMCapable%
HKR, NDI\params\WMMCapable,             type,      0, "enum"
HKR, NDI\params\WMMCapable,             default,   0, "0"
HKR, NDI\params\WMMCapable\enum,        0,         0, %Disable%
HKR, NDI\params\WMMCapable\enum,        1,         0, %Enable%

;
; APSDCapable
;
HKR, ,                            APSDCapable,     0, "0"
HKR, NDI\params\APSDCapable,            ParamDesc, 0, %APSDCapable%
HKR, NDI\params\APSDCapable,            type,      0, "enum"
HKR, NDI\params\APSDCapable,            default,   0, "0"
HKR, NDI\params\APSDCapable\enum,       0,         0, %Disable%
HKR, NDI\params\APSDCapable\enum,       1,         0, %Enable%

;
; APSDAC_BE
;
HKR, ,                            APSDAC_BE,       0, "0"
HKR, NDI\params\APSDAC_BE,              ParamDesc, 0, %APSDAC_BE%
HKR, NDI\params\APSDAC_BE,              type,      0, "enum"
HKR, NDI\params\APSDAC_BE,              default,   0, "0"
HKR, NDI\params\APSDAC_BE\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_BE\enum,         1,         0, %Enable%

;
; APSDAC_BK
;
HKR, ,                            APSDAC_BK,       0, "0"
HKR, NDI\params\APSDAC_BK,              ParamDesc, 0, %APSDAC_BK%
HKR, NDI\params\APSDAC_BK,              type,      0, "enum"
HKR, NDI\params\APSDAC_BK,              default,   0, "0"
HKR, NDI\params\APSDAC_BK\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_BK\enum,         1,         0, %Enable%

;
; APSDAC_VI
;
HKR, ,                            APSDAC_VI,       0, "0"
HKR, NDI\params\APSDAC_VI,              ParamDesc, 0, %APSDAC_VI%
HKR, NDI\params\APSDAC_VI,              type,      0, "enum"
HKR, NDI\params\APSDAC_VI,              default,   0, "0"
HKR, NDI\params\APSDAC_VI\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_VI\enum,         1,         0, %Enable%

;
; APSDAC_VO
;
HKR, ,                            APSDAC_VO,       0, "0"
HKR, NDI\params\APSDAC_VO,              ParamDesc, 0, %APSDAC_VO%
HKR, NDI\params\APSDAC_VO,              type,      0, "enum"
HKR, NDI\params\APSDAC_VO,              default,   0, "0"
HKR, NDI\params\APSDAC_VO\enum,         0,         0, %Disable%
HKR, NDI\params\APSDAC_VO\enum,         1,         0, %Enable%

;
; MaxSPLength
;
HKR, ,                            MaxSPLength,     0, "0"
HKR, Default,                     MaxSPLength,     0, "0"
HKR, NDI\params\MaxSPLength,      ParamDesc,       0, %MaxSPLength%
HKR, NDI\params\MaxSPLength,      type,            0, "int"
HKR, NDI\params\MaxSPLength,      default,         0, "0"
HKR, NDI\params\MaxSPLength,      min,             0, "0"
HKR, NDI\params\MaxSPLength,      max,             0, "3"
HKR, NDI\params\MaxSPLength,      step,            0, "1"
HKR, NDI\params\MaxSPLength,      optional,        0, "0"

;
; DLSCapable
;
HKR, ,                            DLSCapable,      0, "0"
HKR, NDI\params\DLSCapable,             ParamDesc, 0, %DLSCapable%
HKR, NDI\params\DLSCapable,             type,      0, "enum"
HKR, NDI\params\DLSCapable,             default,   0, "0"
HKR, NDI\params\DLSCapable\enum,        0,         0, %Disable%
HKR, NDI\params\DLSCapable\enum,        1,         0, %Enable%

;
; SmartScan
;
HKR, ,                            SmartScan,       0, "0"
HKR, NDI\params\SmartScan,              ParamDesc, 0, %SmartScan%
HKR, NDI\params\SmartScan,              type,      0, "enum"
HKR, NDI\params\SmartScan,              default,   0, "0"
HKR, NDI\params\SmartScan\enum,         0,         0, %Disable%
HKR, NDI\params\SmartScan\enum,         1,         0, %Enable%

;
; CarrierDetect
;
HKR, ,                               CarrierDetect,   0, "0"
HKR, NDI\params\CarrierDetect,       ParamDesc,       0, %CarrierDetect%
HKR, NDI\params\CarrierDetect,       type,            0, "enum"
HKR, NDI\params\CarrierDetect,       default,         0, "0"
HKR, NDI\params\CarrierDetect\enum,  0,               0, %Disable%
HKR, NDI\params\CarrierDetect\enum,  1,               0, %Enable%

;
; PSP XLink mode
;
HKR, ,                            PSPXlink,        0, "0"
HKR, NDI\params\PSPXlink,         ParamDesc,       0, %PSPXlink%
HKR, NDI\params\PSPXlink,         type,            0, "enum"
HKR, NDI\params\PSPXlink,         default,         0, "0"
HKR, NDI\params\PSPXlink\enum,    0,               0, %Disable%
HKR, NDI\params\PSPXlink\enum,    1,               0, %Enable%

;
; CCX2 control
;
HKR, ,                            CCX2Control,     0x00010001, 0x00fa4600

;
; Vendor Description
;
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_DEF_STR%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_DEF_STR%

;
; WPS Device Name
;
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_DEF_STR%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_DEF_STR%

;
; W53 Control
;
HKR, ,                            W53Control,       0, "0"

;*******************************************************************************************
; Profile

;
; SSID
;
;HKR, ,                            SSID,            0, %SSID_DEF_STR%
;HKR, Default,                     SSID,            0, %SSID_DEF_STR%
;HKR, NDI\params\SSID,             ParamDesc,       0, "SSID"
;HKR, NDI\params\SSID,             type,            0, "edit"
;HKR, NDI\params\SSID,             limitText,       0, "32"
;HKR, NDI\params\SSID,             default,         0, %SSID_DEF_STR%

;
; Network Type
;
HKR, ,                            NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, Default,                     NetworkType,     0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType,      ParamDesc,       0, %NetworkType%
HKR, NDI\params\NetworkType,      type,            0, "enum"
HKR, NDI\params\NetworkType,      default,         0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0,               0, %AdHoc%
HKR, NDI\params\NetworkType\enum, 1,               0, %Infrastructure%

;
; Channel
;
HKR, ,                            Channel,         0, %CHANNEL%
HKR, Default,                     Channel,         0, %CHANNEL%


;*******************************************************************************************
; System Configuration Page

;
; Local Administration MAC Network Address
;
HKR, ,                            NetworkAddress,  0, ""
HKR, Default,                     NetworkAddress,  0, ""
HKR, NDI\params\NetworkAddress,   ParamDesc,       0, %LocalNetworkAddress%
HKR, NDI\params\NetworkAddress,   type,            0, "edit"
HKR, NDI\params\NetworkAddress,   limitText,       0, "12"
HKR, NDI\params\NetworkAddress,   default,         0, ""
HKR, NDI\params\Networkaddress,   optional,        0,  "1"

;
; Power Saving Mode
;
HKR, ,                            PSMode,          0, "0"
HKR, Default,                     PSMode,          0, "0"
HKR, NDI\params\PSMode,           ParamDesc,       0, %PSMode%
HKR, NDI\params\PSMode,           type,            0, "enum"
HKR, NDI\params\PSMode,           default,         0, "0"
HKR, NDI\params\PSMode\enum,      0,               0, %CAM%
HKR, NDI\params\PSMode\enum,      1,               0, %MAXPSP%

;
; Preamble Type
;
HKR, ,                            PreambleType,    0, "0"
HKR, Default,                     PreambleType,    0, "0"

;
; RTS Threshold
;
HKR, ,                            RTSThresh,       0, "2347"
HKR, Default,                     RTSThresh,       0, "2347"
HKR, NDI\params\RTSThresh,        ParamDesc,       0, %RTSThresh%
HKR, NDI\params\RTSThresh,        type,            0, "int"
HKR, Ndi\params\RTSThresh,        default,         0, "2347"
HKR, NDI\params\RTSThresh,        min,             0, "0"
HKR, NDI\params\RTSThresh,        max,             0, "2347"
HKR, NDI\params\RTSThresh,        step,            0, "1"
HKR, NDI\params\RTSThresh,        optional,        0, "0"

;
; Fragment Threshold
;
HKR, ,                            FragThresh,      0, "2346"
HKR, Default,                     FragThresh,      0, "2346"
HKR, NDI\params\FragThresh,       ParamDesc,       0, %FragThresh%
HKR, NDI\params\FragThresh,       type,            0, "int"
HKR, Ndi\params\FragThresh,       default,         0, "2346"
HKR, NDI\params\FragThresh,       min,             0, "256"
HKR, NDI\params\FragThresh,       max,             0, "2346"
HKR, NDI\params\FragThresh,       step,            0, "1"
HKR, NDI\params\FragThresh,       optional,        0, "0"

;*******************************************************************************************
; Authentication & Security Page

;
; Authentication Type
;
HKR, ,                AuthenType,      0, "0" ; Open System
HKR, Default,         AuthenType,      0, "0"

;
; Encryption
;
HKR, ,                Encryption,      0, "1" ; Disable
HKR, Default,         Encryption,      0, "1"

;
; WEP Keys Length
;
HKR, ,                WEPKeyLen,       0, "0"
HKR, Default,         WEPKeyLen,       0, "0"

;
; WEP Key to use
;
HKR, ,                WEPKeyUse,       0,"1"
HKR, Default,         WEPKeyUse,       0,"1"

;
; WEP Key1
;
HKR, ,                WEPKey1,         0,""
HKR, Default,         WEPKey1,         0,""

;
; WEP Key2
;
HKR, ,                WEPKey2,         0,""
HKR, Default,         WEPKey2,         0,""

;
; WEP Key3
;
HKR, ,                WEPKey3,         0,""
HKR, Default,         WEPKey3,         0,""

;
; WEP Key4
;
HKR, ,                WEPKey4,         0,""
HKR, Default,         WEPKey4,         0,""

[Customer1.reg]
; Vendor Description
HKR, ,                            VendorDesc,      0, %VENDOR_DESC_CUSTOMER1%
HKR, Default,                     VendorDesc,      0, %VENDOR_DESC_CUSTOMER1%
; WPS Device Name
HKR, ,                            WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%
HKR, Default,                     WPSDevName,      0, %WPS_DEVNAME_CUSTOMER1%

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************

[DestinationDirs]
NT.CopyFiles            = 12    ; system32\drivers subdirectory on NT
XP.CopyFiles            = 12    ; system32\drivers subdirectory on Windows XP

[NT.CopyFiles]
rt61.sys                        ; NT Installation

[XP.CopyFiles]
rt61.sys                        ; XP Installation

[SourceDisksNames]
1                       = %INSTALL_DISK_STR%,,,

[SourceDisksFiles] 
rt61.sys                = 1

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[RT61.ndi.NT.reg]
HKR, Ndi,                   Service,            0, "RT61"
HKR, Ndi\Interfaces,        UpperRange,         0, "ndis5"
HKR, Ndi\Interfaces,        LowerRange,         0, "ethernet"

[General.Service]
DisplayName                 = %General.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[RALINK.Service]
DisplayName                 = %RALINK.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[GIGABYTE.Service]
DisplayName                 = %GIGABYTE.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[Edimax.Service]
DisplayName                 = %EDIMAX.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SITECOM.Service]
DisplayName                 = %SITECOM.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[DELTA.Service]
DisplayName                 = %DELTA.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[HAWKING.Service]
DisplayName                 = %HAWKING.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[BILLIONTON.Service]
DisplayName                 = %BILLIONTON.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[ASUS.Service]
DisplayName                 = %ASUS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[ZINWELL.Service]
DisplayName                 = %ZINWELL.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[AMIT.Service]
DisplayName                 = %AMIT.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[CASTLENET.Service]
DisplayName                 = %CASTLENET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[WN4306A.Service]
DisplayName                 = %WN4306A.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SURECOM.Service]
DisplayName                 = %Surecom.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[BELKIN.Service]
DisplayName                 = %BELKIN.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[VTECH.Service]
DisplayName                 = %VTECH.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SIEMENS.Service]
DisplayName                 = %SIEMENS.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[CONCEPTRONIC.Service]
DisplayName                 = %CONCEPTRONIC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[SMC.Service]
DisplayName                 = %SMC.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[CNET.Service]
DisplayName                 = %CNET.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[COREGA.Service]
DisplayName                 = %COREGA.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[NETOPIA.Service]
DisplayName                 = %NETOPIA.Service.DispName%
ServiceType                 = 1                             ;%SERVICE_KERNEL_DRIVER%
StartType                   = 3                             ;%SERVICE_AUTO_START%
ErrorControl                = 1                             ;%SERVICE_ERROR_NORMAL%
ServiceBinary               = %12%\RT61.sys
LoadOrderGroup              = NDIS

[common.EventLog]
AddReg=common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT61.sys"
HKR, , TypesSupported,   0x00010001, 7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[Strings]
Ralink                      = "Ralink Technology Corp."
Gigabyte                    = "Gigabyte Technology Corp."
Edimax                      = "Edimax Technology Co., Ltd."
Sitecom                     = "Sitecom Europe BV"
Billionton                  = "Billionton Systems Inc."
Delta                       = "Delta Networks, Inc."
Hawking                     = "Hawking Technologies, Inc."
Asus                        = "ASUSTeK Computer Inc."
ZINWELL                     = "ZINWELL Technology, Inc."
AMIT                        = "AMIT Technology, Inc."
CASTLENET                   = "CastleNet Technology, Inc."
ACCTON                      = "Accton Technology Corporation"
Surecom                     = "SURECOM Technology Corp."
Belkin                      = "Belkin Components"
VTech                       = "VTech Telecommunications Ltd"
Siemens                     = "Siemens"
Conceptronic                = "2L (Conceptronic)"
SMC                         = "SMC Networks Inc."
CNet                        = "CNet Technology Inc."
Corega                      = "Corega Components"
Netopia                     = "Netopia, Inc."
AboCom                      = "AboCom Systems, Inc."
Planex                      = "Planex Communications, Inc."
Logitec                     = "Logitec Corporation"
Corega2                     = "Corega K.K."

;*******************************************************************************************
; Device description
;*******************************************************************************************
Ralink_0301.DeviceDesc      = "Ralink Turbo Wireless LAN Card"
Ralink_0302.DeviceDesc      = "Ralink Wireless LAN Card V2"
Ralink_0401.DeviceDesc      = "Ralink MIMO Wireless LAN Card"

GigabyteWM01GS.DeviceDesc   = "Gigabyte GN-WM01GS Cardbus WLAN Card(Turbo)"
GigabyteWI01GS.DeviceDesc   = "Gigabyte GN-WI01GS mini PCI WLAN Card(Turbo)"
GigabyteWP01GS.DeviceDesc   = "Gigabyte GN-WP01GS PCI WLAN Card(Turbo)"
GigabyteWM02GS.DeviceDesc   = "Gigabyte GN-WM01GS Cardbus WLAN Card"
GigabyteWI02GS.DeviceDesc   = "Gigabyte GN-WI01GS mini PCI WLAN Card"
GigabyteWP02GS.DeviceDesc   = "Gigabyte GN-WP01GS PCI WLAN Card"
GigabyteWI02GM.DeviceDesc   = "Gigabyte GN-WI02GM mini PCI MIMO WLAN Card"
GigabyteWM01GM.DeviceDesc   = "Gigabyte GN-WM01GM Cardbus MIMO WLAN Card"
GigabyteWP01GM.DeviceDesc   = "Gigabyte GN-WP01GM PCI MIMO WLAN Card"

EW-0301-7108.DeviceDesc     = "Edimax 802.11g Wireless Cardbus"
EW-0301-7128.DeviceDesc     = "Edimax 802.11g Wireless PCI Card"
EW-7108.DeviceDesc          = "Edimax EW-7108 Series 802.11g Wireless LAN PC Card"
EW-7128.DeviceDesc          = "Edimax EW-7128 Series 802.11g Wireless LAN PCI Card"
EW-7608.DeviceDesc          = "Edimax MIMO Wireless LAN Carbus"
EW-7628.DeviceDesc          = "Edimax MIMO Wireless LAN PCI Card"

GMIWLGRL2-B.DeviceDesc      = "Billionton mini PCI Wireless Lan 11B/G card"
GMIWLGRL2-N.DeviceDesc      = "mini PCI Wireless Lan 11B/G card"

Sitecom_WL112V2.DeviceDesc  = "Sitecom Wireless Network PC Card 54G WL-112v2"
Sitecom_WL115V2.DeviceDesc  = "Sitecom Wireless Network PCI Adapter 54G WL-115v2"
Sitecom_WL170.DeviceDesc    = "Sitecom Wireless Network PC Card turbo g WL-170"
Sitecom_WL171.DeviceDesc    = "Sitecom Wireless Network PCI Card turbo g WL-171"
Sitecom_WL211.DeviceDesc    = "Sitecom Wireless Network 54G-Turbo WPS PCI adapter WL-211"
Sitecom_WL210.DeviceDesc    = "Sitecom Wireless Network 54G-Turbo WPS Cardbus adapter WL-210"
Sitecom_WL150.DeviceDesc    = "Sitecom Wirless Network PC Card MiMoXR WL-150"
Sitecom_WL151.DeviceDesc    = "Sitecom Wireless Network PCI Adapter MiMoXR WL-151"

DeltaPCI.DeviceDesc         = "IEEE 802.11g Wireless PCI Adapter"
DeltaCB.DeviceDesc          = "IEEE 802.11g Wireless PC Card"

Hawking0C54.DeviceDesc      = "Hawking HWC54GR Hi-Speed Wireless-G CardBus Card"
Hawking0B54.DeviceDesc      = "Hawking HWP54GR Hi-Speed Wireless-G PCI Card"

ASUS_837E.DeviceDesc        = "ASUS 802.11 g/b Wireless PCI Adapter"
ASUS.DeviceDesc             = "ASUS 802.11b/g Wireless LAN Card"
ASUSGEN.DeviceDesc          = "802.11b/g Wireless LAN Card"

ZINWELLPCI.DeviceDesc       = "802.11g WLAN PCI Adapter"
ZINWELLMPCI.DeviceDesc      = "802.11g WLAN mini-PCI Adapter"
ZINWELLCARD.DeviceDesc      = "802.11g WLAN CardBus Adapter"
ZINWELLOEM1.DeviceDesc      = "AT&T Plug&Share 54 Mbps Wireless PCI Adapter"
ZINWELLOEM2.DeviceDesc      = "AT&T Plug&Share 54 Mbps Wireless Cardbus Adapter"

AMIT.DeviceDesc             = "AMIT 802.11 g Wireless LAN PC Card"
AMITMINI.DeviceDesc         = "AMIT MINI 802.11 g Wireless LAN PC Card"
AMITPCI.DeviceDesc          = "AMIT PCI 802.11 g Wireless LAN PC Card"
AMIT0100.DeviceDesc         = "802.11g MIMO Wireless Mini-PCI Adapter"
AMIT0200.DeviceDesc         = "802.11g MIMO Wireless Cardbus Adapter"
AMIT0300.DeviceDesc         = "802.11g MIMO Wireless PCI Adapter"
AMIT0202.DeviceDesc         = "AirLive MIMO-G Wireless Cardbus Adapter"
AMIT0302.DeviceDesc         = "AirLive MIMO-G Wireless PCI Adapter"
AMIT0203.DeviceDesc         = "802.11g MIMO Wireless Cardbus Adapter"
AMIT0303.DeviceDesc         = "802.11g MIMO Wireless PCI Adapter"
AMIT0204.DeviceDesc         = "802.11g MIMO Wireless Cardbus Adapter"
AMIT0304.DeviceDesc         = "802.11g MIMO Wireless PCI Adapter"
AMITCG.DeviceDesc           = "CG-WLCBGMO, corega MISO Wireless Cardbus Adapter"
AMIT0006.DeviceDesc         = "CG-WLPCIGMO, corega MISO Wireless PCI Adapter"

CASTLENET.DeviceDesc        = "CastleNet WP1280 802.11 g Wireless LAN Card"

WN4306A.DeviceDesc          = "802.11g 54Mbps Wireless PC Card SE"

SurecomPCI.DeviceDesc       = "802.11g Wireless LAN PCI Adapter"
SurecomCardbus.DeviceDesc   = "802.11g 54M Wireless CardBus Adapter"

Belkin.DeviceDesc           = "Belkin 802.11g Wireless Card"
Belkin_901B.DeviceDesc      = "Belkin Wireless G Plus MIMO Notebook Card"
Belkin_901C.DeviceDesc      = "Belkin Wireless G Plus MIMO Notebook Card"
Belkin_700E.DeviceDesc      = "Belkin Wireless G PCI Adapter"
Belkin_701E.DeviceDesc      = "Belkin Wireless G Notebook Card"

VTechPCI.DeviceDesc         = "VTech Wireless 802.11g PCI Adapter"
VTechCARD.DeviceDesc        = "VTech Wireless 802.11g PCMCIA Adapter"

Siemens.DeviceDesc           = "Siemens 802.11g PC Card Wireless Network Adapter"

Qcom.DeviceDesc             = "Ralink Wireless LAN Card V2"

M61_B833T.DeviceDesc        = "802.11g MiniPCI Turbo Wireless Adapter"
M61_B834T.DeviceDesc        = "802.11g PCI Turbo Wireless Adapter"
M61_B835T.DeviceDesc        = "802.11g CardBus Turbo Wireless Adapter"
M61_B833.DeviceDesc         = "802.11g MiniPCI Wireless Adapter"
M61_B834.DeviceDesc         = "802.11g PCI Wireless Adapter"
M61_B835.DeviceDesc         = "802.11g CardBus Wireless Adapter"
M61_C855.DeviceDesc         = "802.11b/g MiniPCI Wireless Adapter"

WLANm.DeviceDesc            = "WLAN 802.11g miniPCI module"
WLANc.DeviceDesc            = "WLAN 802.11g Cardbus module"

Amigo_9142.DeviceDesc       = "Turbo Wireless PC Card"
Amigo_9222.DeviceDesc       = "Turbo Wireless miniPCI Adapter"
Amigo_9262.DeviceDesc       = "Turbo Wireless PCI Adapter"
AMIGO_9142V2.DeviceDesc     = "802.11G Wireless PC Card"
Amigo_9221.DeviceDesc       = "802.11G Wireless miniPCI Adapter"
Amigo_9261.DeviceDesc       = "802.11G Wireless PCI Adapter"
Amigo_9223.DeviceDesc       = "MIMO Wireless miniPCI Adapter"

CNetPCI.DeviceDesc          = "802.11a/g Wireless LAN PCI"
CNetMPCI.DeviceDesc         = "802.11a/g Wireless LAN Mini-PCI"
CNetCardbus.DeviceDesc      = "802.11a/g Wireless LAN CardBus"

Conceptronic_PCCard.DeviceDesc = "Conceptronic 54g Wireless PC-Card"
Conceptronic_PCICard.DeviceDesc = "Conceptronic 54g Wireless PCI Card"

SMC_EE04.DeviceDesc         = "SMC SMCWCB-GM EZ Connect TM 802.11g Wireless Cardbus Adapter with MIMO Technology"
SMC_EE05.DeviceDesc         = "SMC SMCWPCI-GM EZ Connect TM 802.11g Wireless PCI Adapter with MIMO Technology"

CNet_6221.DeviceDesc        = "CNet Turbo Wireless-G PCI Adapter"
CNet_7221.DeviceDesc        = "CNet Turbo Wireless-G miniPCI Adapter"
CNet_8221.DeviceDesc        = "CNet Turbo Wireless-G Cardbus Adapter"
CNet_6121.DeviceDesc        = "CNet Wireless-G PCI Adapter"
CNet_7121.DeviceDesc        = "CNet Wireless-G miniPCI Adapter"
CNet_8121.DeviceDesc        = "CNet Wireless-G Cardbus Adapter"
CNet_6321.DeviceDesc        = "CNet Wireless-G PCI Adapter"
CNet_7321.DeviceDesc        = "CNet Wireless-G miniPCI Adapter"
CNet_8321.DeviceDesc        = "CNet Wireless-G Cardbus Adapter"

Corega.DeviceDesc           = "CG-WLCB54AGM"

Netopia.DeviceDesc          = "Wireless PC Card"

AboCom_0301_ABA1.DeviceDesc = "802.11b/g Wireless LAN miniPCI Card"
AboCom_0301_ABA2.DeviceDesc = "802.11b/g High Power Wireless LAN miniPCI Card"
AboCom_0301_ABA4.DeviceDesc = "802.11b/g Wireless LAN PCI Card"
AboCom_0301_ABA5.DeviceDesc = "802.11b/g Wireless LAN Cardbus Card"
AboCom_0301_ABE3.DeviceDesc = "802.11a/b/g Wireless LAN miniPCI Card"
AboCom_0301_ABE4.DeviceDesc = "802.11a/b/g High Power Wireless LAN miniPCI Card"
AboCom_0302_ABA1.DeviceDesc = "802.11b/g Wireless LAN miniPCI Card V2"
AboCom_0401_ABA7.DeviceDesc = "PCI MIMO Wireless LAN Card"
AboCom_0401_ABA1.DeviceDesc = "802.11b/g MIMO Wireless LAN miniPCI Card"
AboCom_0401_ABA3.DeviceDesc = "802.11b/g MIMO Wireless LAN miniPCI Card"
AboCom_0401_ABE5.DeviceDesc = "802.11a/b/g MIMO Wireless LAN miniPCI Card"
AboCom_0401_ABA6.DeviceDesc = "802.11b/g MIMO Wireless LAN Cardbus Card"

Planex.DeviceDesc           = "PCI GW-DSMM"

Logitec.DeviceDesc          = "Logitec LAN-WG/CBB Wireless LAN Adapter"

Corega2.DeviceDesc          = "CG-WLCB54GPX"

INSTALL_DISK_STR            = "Ralink Wireless LAN Installation Disk"

General.Service.DispName    = "RT61 Wireless Driver"
RALINK.Service.DispName     = "Ralink RT61 Wireless Driver"
GIGABYTE.Service.DispName   = "Gigabyte RT61 Wireless Driver"
EDIMAX.Service.DispName     = "Edimax RT61 Wireless Driver"
SITECOM.Service.DispName    = "Sitecom RT61 Wireless Network Driver"
DELTA.Service.DispName      = "Delta Networks RT61 Wireless Driver"
HAWKING.Service.DispName    = "Hawking RT61 Wireless Driver"
BILLIONTON.Service.DispName = "Billionton RT61 Wireless Driver"
ASUS.Service.DispName       = "AsusTek RT61 Wireless Driver"
ZINWELL.Service.DispName    = "ZINWELL RT61 Wireless Driver"
AMIT.Service.DispName       = "AMIT RT61 Wireless Driver"
CASTLENET.Service.DispName  = "CastleNet RT61 Wireless Driver"
WN4306A.Service.DispName    = "RT61 802.11g 54Mbps Wireless PC Card SE Driver"
Surecom.Service.DispName    = "Surecom RT61 Wireless Driver"
BELKIN.Service.DispName     = "Belkin RT61 Wireless Driver"
VTECH.Service.DispName      = "VTech RT61 802.11g Wireless Driver"
SIEMENS.Service.DispName    = "Siemens RT61 Wireless 802.11b/g Driver(RT61)"
Conceptronic.Service.DispName = "Conceptronic RT61 54g Wireless Driver"
SMC.Service.DispName        = "SMC RT61 Wireless Driver"
CNET.Service.DispName       = "CNET RT61 Wireless Driver"
COREGA.Service.DispName     = "COREGA Wireless Driver"
NETOPIA.Service.DispName    = "NETOPIA RT61 Wireless Driver"

; Don't put spaces around=sign otherwise installer will not be able to
; find these lines.
;SSID_DEF_STR                = ""
VENDOR_DESC_DEF_STR         = "IEEE 802.11g Wireless Card."
VENDOR_DESC_CUSTOMER1       = "Corega Wireless Card"
NETWORK_TYPE_DEF_STR        = "1"
CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "Ralink Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

RadioOnOff                  = "Radio On/Off"
Disable                     = "Disable"
Enable                      = "Enable"
AutoReconnectMode           = "Auto Reconnect Mode"
CountryRegion24G            = "Country Region 11G"
CountryRegion24G_0          = "#0 (Channel 1 - 11)"
CountryRegion24G_1          = "#1 (Channel 1 - 13)"
CountryRegion24G_2          = "#2 (Channel 10 - 11)"
CountryRegion24G_3          = "#3 (Channel 10 - 13)"
CountryRegion24G_4          = "#4 (Channel 14)"
CountryRegion24G_5          = "#5 (Channel 1 - 14)"
CountryRegion24G_6          = "#6 (Channel 3 - 9)"
CountryRegion24G_7          = "#7 (Channel 5 - 13)"
CountryRegion5G             = "Country Region 11A"
CountryRegion5G_0           = "#0 Ch(36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 Ch(36 - 140)"
CountryRegion5G_2           = "#2 Ch(36 - 64)"
CountryRegion5G_3           = "#3 Ch(52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 Ch(149 - 165)"
CountryRegion5G_5           = "#5 Ch(149 - 161)"
CountryRegion5G_6           = "#6 Ch(36 - 48)"
CountryRegion5G_7           = "#7 Ch(36 - 165)"
CountryRegion5G_8           = "#8 Ch(52 - 64)"
CountryRegion5G_9           = "#9 Ch(34 - 46)"
CountryRegion5G_10          = "#10 Ch(34 - 64)"
BGProtection                = "B/G Protection"
Auto                        = "Auto"
On                          = "On"
Off                         = "Off"
FrameAggregation            = "Frame Aggregation"
IEEE802_11h                 = "IEEE802.11h"
AutoChannelSelect           = "Auto Channel Select"
WMMCapable                  = "WMM Capable"
APSDCapable                 = "APSD Capable"
APSDAC_BE                   = "AC_BE support APSD"
APSDAC_BK                   = "AC_BK support APSD"
APSDAC_VI                   = "AC_VI support APSD"
APSDAC_VO                   = "AC_VO support APSD"
MaxSPLength                 = "Max Service Period Length"
DLSCapable                  = "DLS Capable"
SmartScan                   = "SmartScan"
CarrierDetect               = "Carrier Detect"
PSPXlink                    = "PSP Xlink Mode"
NetworkType                 = "Network Type"
AdHoc                       = "802.11 Ad Hoc"
Infrastructure              = "Infrastructure"
LocalNetworkAddress         = "Local Administration MAC Network Address"
PSMode                      = "Power Saving Mode"
CAM                         = "CAM (Constantly Awake Mode)"
MAXPSP                      = "Max_PSP (Max Power Savings)"
RTSThresh                   = "RTS Threshold"
FragThresh                  = "Fragment Threshold"
