# VIA /S3G Graphics Display Driver Installation Guide for Windows

Updated: 2006-11-23

· Introduction
· License Agreement
· Requirements
– Hardware
– Operating Systems
· Installation
– Windows normal mode
– Silent mode
· Removal
· Language Support

## Introduction

This VIA /S3G Graphics Display Driver Installation Package will install display drivers and related utilities for the UniChrome IGP and DeltaChrome IGP families of integrated graphics processors manufactured by VIA Technologies.

The installation package may be provided either as a compressed .zip file, or as a self-extracting executable .exe file.

## License Agreement

Please read carefully before you download, install, or use any VIA SOFTWARE. VIA SOFTWARE is defined as and includes the software program you are currently trying to download, and all related updates supplied by VIA Technologies, Inc. (VIA). By clicking on the I ACCEPT button, and by downloading and installing the VIA SOFTWARE, you accept all the terms and conditions of this Agreement. If you do not agree to the terms and conditions of this Agreement, do not click the I ACCEPT button or use the VIA SOFTWARE.
Upon your acceptance of this Agreement, subject to the terms and conditions set forth herein, VIA hereby grants to you a limited, non-exclusive, non-transferable, worldwide license to use the VIA SOFTWARE as follows:

Use of Software. The VIA SOFTWARE is licensed for personal use and may only be used in conjunction with VIA products. If you wish to use the VIA SOFTWARE for commercial or any other purpose, please contact VIA directly.
Restrictions. You are not allowed to modify, disassemble, decompile, or reverse-engineering the VIA SOFTWARE, or remove any proprietary notice or label on the VIA SOFTWARE. You may not transfer or distribute this software to any third party.
Ownership and Copyrights. The VIA SOFTWARE and the accompanying documentation are licensed, not sold, to you. All title and copyrights in and to the VIA SOFTWARE (including but not limited to all images, photographs, animations, video, audio, music, text, and other information incorporated into the VIA SOFTWARE), the accompanying printed materials, and any copies of the VIA SOFTWARE, are owned by VIA, or its third party suppliers. The VIA SOFTWARE is protected by copyright laws and international treaty provisions.
Disclaimer of Warranty. VIA MAKES NO REPRESENTATIONS ABOUT THE SUITABILITY, USE, OR PERFORMANCE OF THE VIA SOFTWARE FOR ANY PURPOSE. THE VIA SOFTWARE IS PROVIDED "AS IS," AND VIA DISCLAIMS, TO THE MAXIMUM EXTENT ALLOWED BY APPLICABLE LAW, ALL EXPRESS OR IMPLIED WARRANTIES INCLUDING, BUT NOT LIMITED TO, ANY IMPLIED WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, OR NONINFRINGEMENT WITH RESPECT TO THE VIA SOFTWARE. VIA IS NOT OBLIGATED TO SUPPORT OR ISSUE UPDATES TO THE VIA SOFTWARE.
Limitation on Liability. TO THE MAXIMUM EXTENT ALLOWED BY APPLICABLE LAW, UNDER NO CIRCUMSTANCES SHALL VIA BE LIABLE TO YOU OR ANY OTHER PERSON FOR ANY DIRECT, INDIRECT, SPECIAL, INCIDENTAL, OR CONSEQUENTIAL DAMAGES OF ANY CHARACTER INCLUDING, WITHOUT LIMITATION, DAMAGES FOR LOSS OF GOODWILL, WORK STOPPAGE, COMPUTER FAILURE OR MALFUNCTION, OR ANY AND ALL OTHER ECONOMIC LOSS OR COMMERCIAL DAMAGES ARISING OUT OF THE USE OR INABILITY TO USE THIS VIA SOFTWARE, EVEN IF VIA HAVE BEEN INFORMED OF THE POSSIBILITY OF SUCH DAMAGES.
Export Controls. By clicking on the "I ACCEPT" button, you agree that the VIA Software will not be shipped, transferred, or exported into any country or used in any manner prohibited by the United States Export Administration Act or any other applicable export laws, restrictions, or regulations.
Termination. Your license will automatically terminate without notice from VIA upon any failure by you to comply with the terms under this Agreement. Upon termination, you must cease all use of the VIA SOFTWARE and destroy the VIA SOFTWARE along with all copies and merged portions in any form.

Back to top

## Requirements

### Hardware

This VIA /S3G Graphics Driver Package is compatible with the following integrated graphics processors:

> • Unichrome IGP
> – CLE266
> – KM400
> – P4M800
> • UniChrome Pro IGP
> – CN400
> – CN700
> – K8M800 / K8N800
> – PM800 / PN800
> – P4M800 Pro
> – VN800

> - P4M890

> - VN890

> • Unichrome Pro II IGP
> – CX700
> – CX700M
> – VX700
> • Chrome9 HC IGP

> - K8M890 CE / K8N890 CE

> - P4M900

> - VN896

### Operating Systems

This software package supports the Microsoft Windows Platforms listed below. The setup program will detect the current platform and install the proper driver on your system.

> • Windows 2000 — RTM and above
> • Windows XP — RTM and above
> • Windows Media Center — RTM and above
> • Windows Server 2003 — RTM and above

> • Windows Vista

Back to top

## Installation

The installation package may be provided either as a compressed .zip file, or as a self-extracting executable .exe file.

Note: This package should be installed on a system which has a VIA /S3G graphics chipset. The setup program will automatically terminate without installing if a VIA / S3G graphics chipset is not present.

Two installation modes are provided.

### Windows normal mode

The normal mode executes through a Windows user interface which provides convenient and systematic installation.

> If your download package was in .ZIP format:
> • Double-click the ZIP compressed file and expand it to a folder on your hard disk.
> • Locate the SETUP.EXE file in the folder containing your expanded package.
> • Double-click SETUP to launch the installation program.
> • Respond to the prompts.
> If your download package was in .EXE format:
> • Double-click the self-extracting .EXE execution file.
> • Wait while the file self-extracts. The SETUP tool will launch the installation program automatically.
> • Respond to any requested prompts.
> • The extracted file will be deleted automatically after setup has been terminated.

### Silent mode

In silent install mode the user runs SETUP.EXE from a command line and appends desired parameters to suppress the need for further user intervention. Silent install mode is usually applied by a systems maintenance engineer, as it is a useful mode for servicing a large number of systems that do not have or do not require an interactive user interface. Silent install mode can be run through the command line in console or batch file execution.

The parameters below allow run the setup program to run in silent mode without displaying the popup and dialog windows which might require user input.

Available command line parameters are: -s and -s noreboot ;

> Parameter -s noreboot Description:
> This command line parameter is required to enable silent mode operation. If this parameter is missed, SETUP.EXE will launch the Windows user interface and prompts will require responses from the user.
> Example: setup.exe -s noreboot
> Perform a silent install of the graphics driver and utilities, but do not reboot the computer.
> Parameter -s ; Description:
> This string passes the predefined sub-parameter reboot to SETUP.EXE. Setup -s causes Setup.exe to reboot automatically after the silent mode installation operation is completed.
> Example: setup.exe -s
> Perform a silent install of the graphics driver and utilities, and then reboot the computer.

Note that the command line syntax will differ slightly depending on the downloadable package format, the state of its expansion, and the desire to use batch execution.
For example, a ZIP-Compressed file might be expanded and setup run using a batch file which would include two commands: one to unzip the file and the next to launch setup with the desired parameters. First know where your command-line unzip utility (such as unzip.exe or wzunzip.exe) resides, or include the utility in your path.

Open a command window.
Make a target folder: md targetfolder
Change to the source folder: cd sourcefolder
Unzip the source file to the target folder:
C:\program files\winzip\wzunzip filename.zip C:\targetfolder
Change to the target folder: cd targetfolder
Launch the setup tool with desired parameters: setup.exe -s

The .EXE file could be run directly from the command line using the syntax:

filename.exe -s.

Back to top

## Driver Removal

Click Start, then click Settings, Control Panel.
Double-click Add or Remove Programs.
Scroll through the list of programs available and click the VIA/S3G Display Driver item.
Click Remove. This launches the VIA / S3G Display Driver Uninstall window.
Click Yes to uninstall.

Back to top

## Language Support

This installation package supports the 16 languages listed below.

> Double byte character set languages:
> • Chinese(Simplified) • Chinese (Traditional) • Japanese • Korean •
> Single byte character set languages:
> • Danish • Dutch • English • French • Finish • German • Italian • Norwegian • Portuguese(Brazilian) • Russian • Spanish • Swedish •

If the package is run from a localized version of the Windows operation system and that language is not supported by the installation package, the user interface will be in English.

Back to top

© 2006 VIA Technologies, Inc. All rights reserved.
http://www.via.com.tw/