Software Data Protection Command:
None    = Do not use Software Data Protection. Meant for EEPROMs that do not support SDP.

Enable  = Write protects the EEPROM after flashing. Software Data Protection should always be enabled if EEPROM supports it.

Disable = Disables Software Data Protection after flashing.